<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>8-bit serial-in, serial or parallel-out shift register with output latches and 3-state outputs. Separate shift and storage register clocks (SHCP/STCP) allow gated update of the parallel outputs, and Q7S enables cascading. Wide 2.0-6.0 V CMOS supply, ~100 MHz typical shift-out frequency.</description>
<packages>
<package name="74HC595BQ">
  <description>74HC595BQ</description>
</package>
</packages>
<symbols>
<symbol name="74HC595BQ">
  <pin name="Q1" direction="out"/>
  <pin name="Q2" direction="out"/>
  <pin name="Q3" direction="out"/>
  <pin name="Q4" direction="out"/>
  <pin name="Q5" direction="out"/>
  <pin name="Q6" direction="out"/>
  <pin name="Q7" direction="out"/>
  <pin name="Q7S" direction="out"/>
  <pin name="DS" direction="in"/>
  <pin name="Q0" direction="out"/>
  <pin name="GND" direction="pwr"/>
  <pin name="MR" direction="in"/>
  <pin name="OE" direction="in"/>
  <pin name="SHCP" direction="in"/>
  <pin name="STCP" direction="in"/>
  <pin name="VCC" direction="pwr"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="74HC595BQ" prefix="U">
  <description>8-bit serial-in, serial or parallel-out shift register with output latches and 3-state outputs. Separate shift and storage register clocks (SHCP/STCP) allow gated update of the parallel outputs, and Q7S enables cascading. Wide 2.0-6.0 V CMOS supply, ~100 MHz typical shift-out frequency.</description>
  <gates>
    <gate name="G$1" symbol="74HC595BQ"/>
  </gates>
  <devices>
    <device name="" package="74HC595BQ">
      <connects>
        <connect gate="G$1" pin="Q1" pad="1"/>
        <connect gate="G$1" pin="Q2" pad="2"/>
        <connect gate="G$1" pin="Q3" pad="3"/>
        <connect gate="G$1" pin="Q4" pad="4"/>
        <connect gate="G$1" pin="Q5" pad="5"/>
        <connect gate="G$1" pin="Q6" pad="6"/>
        <connect gate="G$1" pin="Q7" pad="7"/>
        <connect gate="G$1" pin="Q7S" pad="9"/>
        <connect gate="G$1" pin="DS" pad="14"/>
        <connect gate="G$1" pin="Q0" pad="15"/>
        <connect gate="G$1" pin="GND" pad="8"/>
        <connect gate="G$1" pin="MR" pad="10"/>
        <connect gate="G$1" pin="OE" pad="13"/>
        <connect gate="G$1" pin="SHCP" pad="11"/>
        <connect gate="G$1" pin="STCP" pad="12"/>
        <connect gate="G$1" pin="VCC" pad="16"/>
      </connects>
      <technologies><technology name=""/></technologies>
    </device>
  </devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>