<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>BQ76920 3-to-5 series cell battery monitor and analog front-end (AFE) for Li-Ion and phosphate battery packs. Provides cell voltage / pack current / thermistor sensing, integrated cell balancing FETs, hardware overvoltage / undervoltage / overcurrent / short-circuit protection, and an I2C interface to a host controller. The &apos;03&apos; variant is configured for I2C address 0x08, a 3.3-V LDO output, and no CRC on the I2C bus.</description>
<packages>
<package name="BQ7692003">
  <description>BQ7692003</description>
</package>
</packages>
<symbols>
<symbol name="BQ7692003">
  <pin name="TS1" direction="in"/>
  <pin name="VC5" direction="in"/>
  <pin name="VC4" direction="in"/>
  <pin name="VC3" direction="in"/>
  <pin name="VC2" direction="in"/>
  <pin name="VC1" direction="in"/>
  <pin name="VC0" direction="in"/>
  <pin name="SRP" direction="in"/>
  <pin name="SRN" direction="in"/>
  <pin name="NC" direction="nc"/>
  <pin name="DSG" direction="out"/>
  <pin name="CHG" direction="out"/>
  <pin name="VSS" direction="pwr"/>
  <pin name="SDA" direction="io"/>
  <pin name="SCL" direction="in"/>
  <pin name="CAP1" direction="out"/>
  <pin name="REGOUT" direction="out"/>
  <pin name="REGSRC" direction="pwr"/>
  <pin name="BAT" direction="pwr"/>
  <pin name="ALERT" direction="io"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="BQ7692003" prefix="U">
  <description>BQ76920 3-to-5 series cell battery monitor and analog front-end (AFE) for Li-Ion and phosphate battery packs. Provides cell voltage / pack current / thermistor sensing, integrated cell balancing FETs, hardware overvoltage / undervoltage / overcurrent / short-circuit protection, and an I2C interface to a host controller. The &apos;03&apos; variant is configured for I2C address 0x08, a 3.3-V LDO output, and no CRC on the I2C bus.</description>
  <gates>
    <gate name="G$1" symbol="BQ7692003"/>
  </gates>
  <devices>
    <device name="" package="BQ7692003">
      <connects>
        <connect gate="G$1" pin="TS1" pad="6"/>
        <connect gate="G$1" pin="VC5" pad="12"/>
        <connect gate="G$1" pin="VC4" pad="13"/>
        <connect gate="G$1" pin="VC3" pad="14"/>
        <connect gate="G$1" pin="VC2" pad="15"/>
        <connect gate="G$1" pin="VC1" pad="16"/>
        <connect gate="G$1" pin="VC0" pad="17"/>
        <connect gate="G$1" pin="SRP" pad="18"/>
        <connect gate="G$1" pin="SRN" pad="19"/>
        <connect gate="G$1" pin="NC" pad="11"/>
        <connect gate="G$1" pin="DSG" pad="1"/>
        <connect gate="G$1" pin="CHG" pad="2"/>
        <connect gate="G$1" pin="VSS" pad="3"/>
        <connect gate="G$1" pin="SDA" pad="4"/>
        <connect gate="G$1" pin="SCL" pad="5"/>
        <connect gate="G$1" pin="CAP1" pad="7"/>
        <connect gate="G$1" pin="REGOUT" pad="8"/>
        <connect gate="G$1" pin="REGSRC" pad="9"/>
        <connect gate="G$1" pin="BAT" pad="10"/>
        <connect gate="G$1" pin="ALERT" pad="20"/>
      </connects>
      <technologies><technology name=""/></technologies>
    </device>
  </devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>