<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description></description>
<packages>
<package name="ADS8588SIPM">
  <description>ADS8588SIPM</description>
</package>
</packages>
<symbols>
<symbol name="ADS8588SIPM">
  <pin name="AVDD_1" direction="io"/>
  <pin name="AGND_1" direction="io"/>
  <pin name="OS0" direction="io"/>
  <pin name="OS1" direction="io"/>
  <pin name="OS2" direction="io"/>
  <pin name="!PAR!/SER/BYTE_SEL" direction="io"/>
  <pin name="!STBY" direction="io"/>
  <pin name="RANGE" direction="io"/>
  <pin name="CONVSTA" direction="io"/>
  <pin name="CONVSTB" direction="io"/>
  <pin name="RESET" direction="io"/>
  <pin name="!RD!/SCLK" direction="io"/>
  <pin name="!CS" direction="io"/>
  <pin name="BUSY" direction="io"/>
  <pin name="FRSTDATA" direction="io"/>
  <pin name="DB0" direction="io"/>
  <pin name="DB1" direction="io"/>
  <pin name="DB2" direction="io"/>
  <pin name="DB3" direction="io"/>
  <pin name="DB4" direction="io"/>
  <pin name="DB5" direction="io"/>
  <pin name="DB6" direction="io"/>
  <pin name="DVDD" direction="io"/>
  <pin name="DB7/DOUTA" direction="io"/>
  <pin name="DB8/DOUTB" direction="io"/>
  <pin name="AGND_2" direction="io"/>
  <pin name="DB9" direction="io"/>
  <pin name="DB10" direction="io"/>
  <pin name="DB11" direction="io"/>
  <pin name="DB12" direction="io"/>
  <pin name="DB13" direction="io"/>
  <pin name="DB14/HBEN" direction="io"/>
  <pin name="AVDD_4" direction="io"/>
  <pin name="AGND_6" direction="io"/>
  <pin name="REFGND_2" direction="io"/>
  <pin name="REFCAPB" direction="io"/>
  <pin name="REFCAPA" direction="io"/>
  <pin name="REFGND_1" direction="io"/>
  <pin name="REFIN/REFOUT" direction="io"/>
  <pin name="AGND_5" direction="io"/>
  <pin name="AGND_4" direction="io"/>
  <pin name="REGCAP2" direction="io"/>
  <pin name="AVDD_3" direction="io"/>
  <pin name="AVDD_2" direction="io"/>
  <pin name="REGCAP1" direction="io"/>
  <pin name="AGND_3" direction="io"/>
  <pin name="REFSEL" direction="io"/>
  <pin name="DB15/BYTE_SEL" direction="io"/>
  <pin name="AIN_8GND" direction="io"/>
  <pin name="AIN_8P" direction="io"/>
  <pin name="AIN_7GND" direction="io"/>
  <pin name="AIN_7P" direction="io"/>
  <pin name="AIN_6GND" direction="io"/>
  <pin name="AIN_6P" direction="io"/>
  <pin name="AIN_5GND" direction="io"/>
  <pin name="AIN_5P" direction="io"/>
  <pin name="AIN_4GND" direction="io"/>
  <pin name="AIN_4P" direction="io"/>
  <pin name="AIN_3GND" direction="io"/>
  <pin name="AIN_3P" direction="io"/>
  <pin name="AIN_2GND" direction="io"/>
  <pin name="AIN_2P" direction="io"/>
  <pin name="AIN_1GND" direction="io"/>
  <pin name="AIN_1P" direction="io"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="ADS8588SIPM" prefix="U">
  <description></description>
  <gates>
    <gate name="G$1" symbol="ADS8588SIPM"/>
  </gates>
  <devices>
    <device name="" package="ADS8588SIPM">
      <connects>
        <connect gate="G$1" pin="AVDD_1" pad="1"/>
        <connect gate="G$1" pin="AGND_1" pad="2"/>
        <connect gate="G$1" pin="OS0" pad="3"/>
        <connect gate="G$1" pin="OS1" pad="4"/>
        <connect gate="G$1" pin="OS2" pad="5"/>
        <connect gate="G$1" pin="!PAR!/SER/BYTE_SEL" pad="6"/>
        <connect gate="G$1" pin="!STBY" pad="7"/>
        <connect gate="G$1" pin="RANGE" pad="8"/>
        <connect gate="G$1" pin="CONVSTA" pad="9"/>
        <connect gate="G$1" pin="CONVSTB" pad="10"/>
        <connect gate="G$1" pin="RESET" pad="11"/>
        <connect gate="G$1" pin="!RD!/SCLK" pad="12"/>
        <connect gate="G$1" pin="!CS" pad="13"/>
        <connect gate="G$1" pin="BUSY" pad="14"/>
        <connect gate="G$1" pin="FRSTDATA" pad="15"/>
        <connect gate="G$1" pin="DB0" pad="16"/>
        <connect gate="G$1" pin="DB1" pad="17"/>
        <connect gate="G$1" pin="DB2" pad="18"/>
        <connect gate="G$1" pin="DB3" pad="19"/>
        <connect gate="G$1" pin="DB4" pad="20"/>
        <connect gate="G$1" pin="DB5" pad="21"/>
        <connect gate="G$1" pin="DB6" pad="22"/>
        <connect gate="G$1" pin="DVDD" pad="23"/>
        <connect gate="G$1" pin="DB7/DOUTA" pad="24"/>
        <connect gate="G$1" pin="DB8/DOUTB" pad="25"/>
        <connect gate="G$1" pin="AGND_2" pad="26"/>
        <connect gate="G$1" pin="DB9" pad="27"/>
        <connect gate="G$1" pin="DB10" pad="28"/>
        <connect gate="G$1" pin="DB11" pad="29"/>
        <connect gate="G$1" pin="DB12" pad="30"/>
        <connect gate="G$1" pin="DB13" pad="31"/>
        <connect gate="G$1" pin="DB14/HBEN" pad="32"/>
        <connect gate="G$1" pin="AVDD_4" pad="48"/>
        <connect gate="G$1" pin="AGND_6" pad="47"/>
        <connect gate="G$1" pin="REFGND_2" pad="46"/>
        <connect gate="G$1" pin="REFCAPB" pad="45"/>
        <connect gate="G$1" pin="REFCAPA" pad="44"/>
        <connect gate="G$1" pin="REFGND_1" pad="43"/>
        <connect gate="G$1" pin="REFIN/REFOUT" pad="42"/>
        <connect gate="G$1" pin="AGND_5" pad="41"/>
        <connect gate="G$1" pin="AGND_4" pad="40"/>
        <connect gate="G$1" pin="REGCAP2" pad="39"/>
        <connect gate="G$1" pin="AVDD_3" pad="38"/>
        <connect gate="G$1" pin="AVDD_2" pad="37"/>
        <connect gate="G$1" pin="REGCAP1" pad="36"/>
        <connect gate="G$1" pin="AGND_3" pad="35"/>
        <connect gate="G$1" pin="REFSEL" pad="34"/>
        <connect gate="G$1" pin="DB15/BYTE_SEL" pad="33"/>
        <connect gate="G$1" pin="AIN_8GND" pad="64"/>
        <connect gate="G$1" pin="AIN_8P" pad="63"/>
        <connect gate="G$1" pin="AIN_7GND" pad="62"/>
        <connect gate="G$1" pin="AIN_7P" pad="61"/>
        <connect gate="G$1" pin="AIN_6GND" pad="60"/>
        <connect gate="G$1" pin="AIN_6P" pad="59"/>
        <connect gate="G$1" pin="AIN_5GND" pad="58"/>
        <connect gate="G$1" pin="AIN_5P" pad="57"/>
        <connect gate="G$1" pin="AIN_4GND" pad="56"/>
        <connect gate="G$1" pin="AIN_4P" pad="55"/>
        <connect gate="G$1" pin="AIN_3GND" pad="54"/>
        <connect gate="G$1" pin="AIN_3P" pad="53"/>
        <connect gate="G$1" pin="AIN_2GND" pad="52"/>
        <connect gate="G$1" pin="AIN_2P" pad="51"/>
        <connect gate="G$1" pin="AIN_1GND" pad="50"/>
        <connect gate="G$1" pin="AIN_1P" pad="49"/>
      </connects>
      <technologies><technology name=""/></technologies>
    </device>
  </devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>