<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>KOHERelec MDA4020-3R3M molded power inductor, 3.3 uH +/-20 percent, 3.5 A rated, 3.1 A saturation, 65 mohm DCR, 4.5 x 4.1 mm SMD</description>
<packages>
<package name="MDA4020-3R3M">
  <description>MDA4020-3R3M</description>
</package>
</packages>
<symbols>
<symbol name="MDA4020-3R3M">
  <pin name="1" direction="pas"/>
  <pin name="2" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="MDA4020-3R3M" prefix="L">
  <description>KOHERelec MDA4020-3R3M molded power inductor, 3.3 uH +/-20 percent, 3.5 A rated, 3.1 A saturation, 65 mohm DCR, 4.5 x 4.1 mm SMD</description>
  <gates>
    <gate name="G$1" symbol="MDA4020-3R3M"/>
  </gates>
  <devices>
    <device name="" package="MDA4020-3R3M">
      <connects>
        <connect gate="G$1" pin="1" pad="1"/>
        <connect gate="G$1" pin="2" pad="2"/>
      </connects>
      <technologies><technology name=""/></technologies>
    </device>
  </devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>