<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>Texas Instruments TPD2EUSB30DRTR 2-channel TVS ESD protection array for USB 3.0 SuperSpeed (5 Gbps), 0.7 pF typ IO-GND capacitance, IEC 61000-4-2 +/-8 kV contact and air-gap, IEC 61000-4-5 5 A surge, 5.5 V VRWM, 3-pin SOT (DRT) 1.00 x 0.80 mm</description>
<packages>
<package name="TPD2EUSB30DRTR">
  <description>TPD2EUSB30DRTR</description>
</package>
</packages>
<symbols>
<symbol name="TPD2EUSB30DRTR">
  <pin name="D+" direction="pas"/>
  <pin name="D-" direction="pas"/>
  <pin name="GND" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="TPD2EUSB30DRTR" prefix="D">
  <description>Texas Instruments TPD2EUSB30DRTR 2-channel TVS ESD protection array for USB 3.0 SuperSpeed (5 Gbps), 0.7 pF typ IO-GND capacitance, IEC 61000-4-2 +/-8 kV contact and air-gap, IEC 61000-4-5 5 A surge, 5.5 V VRWM, 3-pin SOT (DRT) 1.00 x 0.80 mm</description>
  <gates>
    <gate name="G$1" symbol="TPD2EUSB30DRTR"/>
  </gates>
  <devices>
    <device name="" package="TPD2EUSB30DRTR">
      <connects>
        <connect gate="G$1" pin="D+" pad="1"/>
        <connect gate="G$1" pin="D-" pad="2"/>
        <connect gate="G$1" pin="GND" pad="3"/>
      </connects>
      <technologies><technology name=""/></technologies>
    </device>
  </devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>