<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>\n                        \n                            IC RF TxRx + MCU 802.15.4, Bluetooth Bluetooth v5.4, Matter, Thread, Zigbee® 48-VFQFN Exposed Pad\n                        \n</description>
<packages>
<package name="nRF54L15">
  <description>nRF54L15 placeholder footprint</description>
</package>
</packages>
<symbols>
<symbol name="nRF54L15">
  <pin name="DCC" direction="pwr"/>
  <pin name="DECA" direction="pwr"/>
  <pin name="DECD" direction="pwr"/>
  <pin name="DECRF" direction="pwr"/>
  <pin name="VDD" direction="pwr"/>
  <pin name="VDD@2" direction="pwr"/>
  <pin name="VDD@3" direction="pwr"/>
  <pin name="VDD@4" direction="pwr"/>
  <pin name="VDD@5" direction="pwr"/>
  <pin name="~{RESET}" direction="in"/>
  <pin name="SWDCLK" direction="in"/>
  <pin name="XC1" direction="in"/>
  <pin name="XC2" direction="in"/>
  <pin name="P0.00" direction="io"/>
  <pin name="P0.01" direction="io"/>
  <pin name="P0.02" direction="io"/>
  <pin name="P0.03/GRTCPWM" direction="io"/>
  <pin name="P0.04/GRTCLFCLKOUT" direction="io"/>
  <pin name="P1.00/XL1" direction="io"/>
  <pin name="P1.01/XL2" direction="io"/>
  <pin name="P1.02/NFC1" direction="io"/>
  <pin name="P1.03/NFC2" direction="io"/>
  <pin name="P1.04/ASO(0)/AIN0" direction="io"/>
  <pin name="P1.05/ASI(0)/RADIO(6)/AIN1" direction="io"/>
  <pin name="P1.06/ASO(1)/AIN2" direction="io"/>
  <pin name="P1.07/ASI(1)/AIN3" direction="io"/>
  <pin name="P1.08/CLK16M/EXTREF" direction="io"/>
  <pin name="P1.09/ASO(2)/RADIO(0)" direction="io"/>
  <pin name="P1.10/ASI(2)/RADIO(1)" direction="io"/>
  <pin name="ANT" direction="out"/>
  <pin name="P1.11/ASO(3)/RADIO(2)/AIN4" direction="io"/>
  <pin name="P1.12/ASI(3)/RADIO(3)/AIN5" direction="io"/>
  <pin name="P1.13/RADIO(4)/AIN6" direction="io"/>
  <pin name="P1.14/RADIO(5)/AIN7" direction="io"/>
  <pin name="P2.00" direction="io"/>
  <pin name="P2.01" direction="io"/>
  <pin name="P2.02" direction="io"/>
  <pin name="P2.03" direction="io"/>
  <pin name="P2.04" direction="io"/>
  <pin name="P2.05" direction="io"/>
  <pin name="P2.06/TRACECLK" direction="io"/>
  <pin name="P2.07/TRACEDATA(0)/SWO" direction="io"/>
  <pin name="P2.08/TRACEDATA(1)" direction="io"/>
  <pin name="P2.09/TRACEDATA(2)" direction="io"/>
  <pin name="P2.10/TRACEDATA(3)" direction="io"/>
  <pin name="SWDIO" direction="io"/>
  <pin name="VSS" direction="pwr"/>
  <pin name="VSS@2" direction="pwr"/>
  <pin name="VSS_PA" direction="pwr"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="nRF54L15" prefix="U">
  <description>\n                        \n                            IC RF TxRx + MCU 802.15.4, Bluetooth Bluetooth v5.4, Matter, Thread, Zigbee® 48-VFQFN Exposed Pad\n                        \n</description>
  <gates>
    <gate name="G$1" symbol="nRF54L15"/>
  </gates>
  <devices>
    <device name="" package="nRF54L15">
      <connects>
        <connect gate="G$1" pin="DCC" pad="46"/>
        <connect gate="G$1" pin="DECA" pad="43"/>
        <connect gate="G$1" pin="DECD" pad="45"/>
        <connect gate="G$1" pin="DECRF" pad="33"/>
        <connect gate="G$1" pin="VDD" pad="10"/>
        <connect gate="G$1" pin="VDD@2" pad="22"/>
        <connect gate="G$1" pin="VDD@3" pad="36"/>
        <connect gate="G$1" pin="VDD@4" pad="47"/>
        <connect gate="G$1" pin="VDD@5" pad="48"/>
        <connect gate="G$1" pin="~{RESET}" pad="30"/>
        <connect gate="G$1" pin="SWDCLK" pad="26"/>
        <connect gate="G$1" pin="XC1" pad="34"/>
        <connect gate="G$1" pin="XC2" pad="35"/>
        <connect gate="G$1" pin="P0.00" pad="23"/>
        <connect gate="G$1" pin="P0.01" pad="24"/>
        <connect gate="G$1" pin="P0.02" pad="27"/>
        <connect gate="G$1" pin="P0.03/GRTCPWM" pad="28"/>
        <connect gate="G$1" pin="P0.04/GRTCLFCLKOUT" pad="29"/>
        <connect gate="G$1" pin="P1.00/XL1" pad="1"/>
        <connect gate="G$1" pin="P1.01/XL2" pad="2"/>
        <connect gate="G$1" pin="P1.02/NFC1" pad="3"/>
        <connect gate="G$1" pin="P1.03/NFC2" pad="4"/>
        <connect gate="G$1" pin="P1.04/ASO(0)/AIN0" pad="5"/>
        <connect gate="G$1" pin="P1.05/ASI(0)/RADIO(6)/AIN1" pad="6"/>
        <connect gate="G$1" pin="P1.06/ASO(1)/AIN2" pad="7"/>
        <connect gate="G$1" pin="P1.07/ASI(1)/AIN3" pad="8"/>
        <connect gate="G$1" pin="P1.08/CLK16M/EXTREF" pad="9"/>
        <connect gate="G$1" pin="P1.09/ASO(2)/RADIO(0)" pad="37"/>
        <connect gate="G$1" pin="P1.10/ASI(2)/RADIO(1)" pad="38"/>
        <connect gate="G$1" pin="ANT" pad="31"/>
        <connect gate="G$1" pin="P1.11/ASO(3)/RADIO(2)/AIN4" pad="39"/>
        <connect gate="G$1" pin="P1.12/ASI(3)/RADIO(3)/AIN5" pad="40"/>
        <connect gate="G$1" pin="P1.13/RADIO(4)/AIN6" pad="41"/>
        <connect gate="G$1" pin="P1.14/RADIO(5)/AIN7" pad="42"/>
        <connect gate="G$1" pin="P2.00" pad="11"/>
        <connect gate="G$1" pin="P2.01" pad="12"/>
        <connect gate="G$1" pin="P2.02" pad="13"/>
        <connect gate="G$1" pin="P2.03" pad="14"/>
        <connect gate="G$1" pin="P2.04" pad="15"/>
        <connect gate="G$1" pin="P2.05" pad="16"/>
        <connect gate="G$1" pin="P2.06/TRACECLK" pad="17"/>
        <connect gate="G$1" pin="P2.07/TRACEDATA(0)/SWO" pad="18"/>
        <connect gate="G$1" pin="P2.08/TRACEDATA(1)" pad="19"/>
        <connect gate="G$1" pin="P2.09/TRACEDATA(2)" pad="20"/>
        <connect gate="G$1" pin="P2.10/TRACEDATA(3)" pad="21"/>
        <connect gate="G$1" pin="SWDIO" pad="25"/>
        <connect gate="G$1" pin="VSS" pad="44"/>
        <connect gate="G$1" pin="VSS@2" pad="49"/>
        <connect gate="G$1" pin="VSS_PA" pad="32"/>
      </connects>
      <technologies><technology name=""/></technologies>
    </device>
  </devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>