(kicad_symbol_lib (version 20211014) (generator kicad_symbol_editor)
  (symbol "NRF52840-CKAA-R7" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at -22.8707 35.9661 0))
    (property "Value" "NRF52840-CKAA-R7" (id 1) (at -22.8992 -38.58 0))
    (property "Footprint" "NRF52840-CKAA-R7:BGA94N35P10X10_360X354X51N" (id 2) (at 0 0 0))
    (property "MF" "Nordic Semiconductors" (id 4) (at 0 0 0))
    (property "MAXIMUM_PACKAGE_HEIGHT" "0.514mm" (id 5) (at 0 0 0))
    (property "Package" "None" (id 6) (at 0 0 0))
    (property "Price" "None" (id 7) (at 0 0 0))
    (property "Check_prices" "https://www.snapeda.com/parts/NRF52840-CKAA-R7/Nordic+Power/view-part/?ref=eda" (id 8) (at 0 0 0))
    (property "STANDARD" "IPC7351B" (id 9) (at 0 0 0))
    (property "PARTREV" "1.1" (id 10) (at 0 0 0))
    (property "SnapEDA_Link" "https://www.snapeda.com/parts/NRF52840-CKAA-R7/Nordic+Power/view-part/?ref=snap" (id 11) (at 0 0 0))
    (property "MP" "NRF52840-CKAA-R7" (id 12) (at 0 0 0))
    (property "Description" "\n                        \n                            IC RF TxRx + MCU 802.15.4, Bluetooth Bluetooth v5.0, Thread, Zigbee® 2.4GHz 94-UFBGA, WLCSP\n                        \n" (id 13) (at 0 0 0))
    (property "Availability" "In Stock" (id 14) (at 0 0 0))
    (property "MANUFACTURER" "Nordic" (id 15) (at 0 0 0))
    (symbol "NRF52840-CKAA-R7_1_0"
      (pin bidirectional line (at -27.94 33.02 0) (length 5.08)
        (name "P0.00/XL1")
        (number "B9")
      )
      (pin bidirectional line (at -27.94 30.48 0) (length 5.08)
        (name "P0.01/XL2")
        (number "B10")
      )
      (pin bidirectional line (at -27.94 27.94 0) (length 5.08)
        (name "P0.02/AIN0")
        (number "B6")
      )
      (pin bidirectional line (at -27.94 25.4 0) (length 5.08)
        (name "P0.03/AIN1")
        (number "A5")
      )
      (pin bidirectional line (at -27.94 22.86 0) (length 5.08)
        (name "P0.04/AIN2")
        (number "C10")
      )
      (pin bidirectional line (at -27.94 20.32 0) (length 5.08)
        (name "P0.05/AIN3")
        (number "D10")
      )
      (pin bidirectional line (at -27.94 17.78 0) (length 5.08)
        (name "P0.06")
        (number "E9")
      )
      (pin bidirectional line (at -27.94 15.24 0) (length 5.08)
        (name "P0.07/TRACECLK")
        (number "F9")
      )
      (pin bidirectional line (at -27.94 12.7 0) (length 5.08)
        (name "P0.08")
        (number "E10")
      )
      (pin bidirectional line (at -27.94 10.16 0) (length 5.08)
        (name "P0.09/NFC1")
        (number "F1")
      )
      (pin bidirectional line (at -27.94 7.62 0) (length 5.08)
        (name "P0.10/NFC2")
        (number "E2")
      )
      (pin bidirectional line (at -27.94 5.08 0) (length 5.08)
        (name "P0.11/TRACEDATA2")
        (number "H8")
      )
      (pin bidirectional line (at -27.94 2.54 0) (length 5.08)
        (name "P0.12/TRACEDATA1")
        (number "G10")
      )
      (pin bidirectional line (at -27.94 0.0 0) (length 5.08)
        (name "P0.13")
        (number "H7")
      )
      (pin bidirectional line (at -27.94 -2.54 0) (length 5.08)
        (name "P0.14")
        (number "J7")
      )
      (pin bidirectional line (at -27.94 -5.08 0) (length 5.08)
        (name "P0.15")
        (number "K7")
      )
      (pin bidirectional line (at -27.94 -7.62 0) (length 5.08)
        (name "P0.16")
        (number "H6")
      )
      (pin bidirectional line (at -27.94 -10.16 0) (length 5.08)
        (name "P0.17")
        (number "J6")
      )
      (pin bidirectional line (at -27.94 -12.7 0) (length 5.08)
        (name "P0.18/~{RESET}")
        (number "K6")
      )
      (pin bidirectional line (at -27.94 -15.24 0) (length 5.08)
        (name "P0.19")
        (number "K4")
      )
      (pin bidirectional line (at -27.94 -17.78 0) (length 5.08)
        (name "P0.20")
        (number "J5")
      )
      (pin bidirectional line (at -27.94 -20.32 0) (length 5.08)
        (name "P0.21")
        (number "J4")
      )
      (pin bidirectional line (at -27.94 -22.86 0) (length 5.08)
        (name "P0.22")
        (number "K3")
      )
      (pin bidirectional line (at -27.94 -25.4 0) (length 5.08)
        (name "P0.23")
        (number "H5")
      )
      (pin bidirectional line (at -27.94 -27.94 0) (length 5.08)
        (name "P0.24")
        (number "H4")
      )
      (pin bidirectional line (at -27.94 -30.48 0) (length 5.08)
        (name "P0.25")
        (number "K2")
      )
      (pin bidirectional line (at -27.94 -33.02 0) (length 5.08)
        (name "P0.26")
        (number "C9")
      )
      (pin bidirectional line (at 27.94 -22.86 180.0) (length 5.08)
        (name "P0.27")
        (number "D9")
      )
      (pin bidirectional line (at 27.94 -25.4 180.0) (length 5.08)
        (name "P0.28/AIN4")
        (number "A6")
      )
      (pin bidirectional line (at 27.94 -27.94 180.0) (length 5.08)
        (name "P0.29/AIN5")
        (number "C7")
      )
      (pin bidirectional line (at 27.94 -30.48 180.0) (length 5.08)
        (name "P0.30/AIN6")
        (number "A7")
      )
      (pin bidirectional line (at 27.94 -33.02 180.0) (length 5.08)
        (name "P0.31/AIN7")
        (number "C8")
      )
      (pin bidirectional line (at 27.94 20.32 180.0) (length 5.08)
        (name "P1.00/TRACEDATA0")
        (number "J3")
      )
      (pin bidirectional line (at 27.94 17.78 180.0) (length 5.08)
        (name "P1.01")
        (number "J1")
      )
      (pin bidirectional line (at 27.94 15.24 180.0) (length 5.08)
        (name "P1.02")
        (number "G3")
      )
      (pin bidirectional line (at 27.94 12.7 180.0) (length 5.08)
        (name "P1.03")
        (number "F3")
      )
      (pin bidirectional line (at 27.94 10.16 180.0) (length 5.08)
        (name "P1.04")
        (number "H1")
      )
      (pin bidirectional line (at 27.94 7.62 180.0) (length 5.08)
        (name "P1.05")
        (number "G2")
      )
      (pin bidirectional line (at 27.94 5.08 180.0) (length 5.08)
        (name "P1.06")
        (number "E3")
      )
      (pin bidirectional line (at 27.94 2.54 180.0) (length 5.08)
        (name "P1.07")
        (number "G1")
      )
      (pin bidirectional line (at 27.94 0.0 180.0) (length 5.08)
        (name "P1.08")
        (number "G9")
      )
      (pin bidirectional line (at 27.94 -2.54 180.0) (length 5.08)
        (name "P1.09//TRACEDATA3")
        (number "F10")
      )
      (pin bidirectional line (at 27.94 -5.08 180.0) (length 5.08)
        (name "P1.10")
        (number "B4")
      )
      (pin bidirectional line (at 27.94 -7.62 180.0) (length 5.08)
        (name "P1.11")
        (number "A3")
      )
      (pin bidirectional line (at 27.94 -10.16 180.0) (length 5.08)
        (name "P1.12")
        (number "C5")
      )
      (pin bidirectional line (at 27.94 -12.7 180.0) (length 5.08)
        (name "P1.13")
        (number "A4")
      )
      (pin bidirectional line (at 27.94 -15.24 180.0) (length 5.08)
        (name "P1.14")
        (number "B5")
      )
      (pin bidirectional line (at 27.94 -17.78 180.0) (length 5.08)
        (name "P1.15")
        (number "C6")
      )
      (pin bidirectional line (at 27.94 33.02 180.0) (length 5.08)
        (name "ANT")
        (number "E1")
      )
      (pin bidirectional line (at 27.94 27.94 180.0) (length 5.08)
        (name "D-")
        (number "J8")
      )
      (pin bidirectional line (at 27.94 25.4 180.0) (length 5.08)
        (name "D+")
        (number "K8")
      )
    )
    (symbol "NRF52840-CKAA-R7_2_0"
      (pin power_in line (at -15.24 -7.62 0) (length 5.08)
        (name "DEC6")
        (number "C2")
      )
      (pin power_in line (at 15.24 7.62 180.0) (length 5.08)
        (name "VDD")
        (number "B3")
      )
      (pin power_in line (at 15.24 7.62 180.0) (length 5.08) hide
        (name "VDD")
        (number "B8")
      )
      (pin power_in line (at 15.24 7.62 180.0) (length 5.08) hide
        (name "VDD")
        (number "H10")
      )
      (pin power_in line (at 15.24 7.62 180.0) (length 5.08) hide
        (name "VDD")
        (number "K1")
      )
      (pin power_in line (at 15.24 7.62 180.0) (length 5.08) hide
        (name "VDD")
        (number "K5")
      )
      (pin power_in line (at -15.24 10.16 0) (length 5.08)
        (name "DCC")
        (number "A9")
      )
      (pin power_in line (at -15.24 0.0 0) (length 5.08)
        (name "DEC1")
        (number "A10")
      )
      (pin power_in line (at -15.24 -2.54 0) (length 5.08)
        (name "DEC4")
        (number "A8")
      )
      (pin power_in line (at 15.24 -2.54 180.0) (length 5.08)
        (name "VSS")
        (number "B7")
      )
      (pin power_in line (at 15.24 -2.54 180.0) (length 5.08) hide
        (name "VSS")
        (number "C4")
      )
      (pin power_in line (at 15.24 -2.54 180.0) (length 5.08) hide
        (name "VSS")
        (number "D3")
      )
      (pin power_in line (at 15.24 -2.54 180.0) (length 5.08) hide
        (name "VSS")
        (number "D4")
      )
      (pin power_in line (at 15.24 -2.54 180.0) (length 5.08) hide
        (name "VSS")
        (number "D5")
      )
      (pin power_in line (at 15.24 -2.54 180.0) (length 5.08) hide
        (name "VSS")
        (number "D6")
      )
      (pin power_in line (at 15.24 -2.54 180.0) (length 5.08) hide
        (name "VSS")
        (number "D7")
      )
      (pin power_in line (at 15.24 -2.54 180.0) (length 5.08) hide
        (name "VSS")
        (number "D8")
      )
      (pin power_in line (at 15.24 -2.54 180.0) (length 5.08) hide
        (name "VSS")
        (number "E4")
      )
      (pin power_in line (at 15.24 -2.54 180.0) (length 5.08) hide
        (name "VSS")
        (number "E5")
      )
      (pin power_in line (at 15.24 -2.54 180.0) (length 5.08) hide
        (name "VSS")
        (number "E6")
      )
      (pin power_in line (at 15.24 -2.54 180.0) (length 5.08) hide
        (name "VSS")
        (number "E7")
      )
      (pin power_in line (at 15.24 -2.54 180.0) (length 5.08) hide
        (name "VSS")
        (number "E8")
      )
      (pin power_in line (at 15.24 -2.54 180.0) (length 5.08) hide
        (name "VSS")
        (number "F4")
      )
      (pin power_in line (at 15.24 -2.54 180.0) (length 5.08) hide
        (name "VSS")
        (number "F5")
      )
      (pin power_in line (at 15.24 -2.54 180.0) (length 5.08) hide
        (name "VSS")
        (number "F6")
      )
      (pin power_in line (at 15.24 -2.54 180.0) (length 5.08) hide
        (name "VSS")
        (number "F7")
      )
      (pin power_in line (at 15.24 -2.54 180.0) (length 5.08) hide
        (name "VSS")
        (number "F8")
      )
      (pin power_in line (at 15.24 -2.54 180.0) (length 5.08) hide
        (name "VSS")
        (number "G4")
      )
      (pin power_in line (at 15.24 -2.54 180.0) (length 5.08) hide
        (name "VSS")
        (number "G5")
      )
      (pin power_in line (at 15.24 -2.54 180.0) (length 5.08) hide
        (name "VSS")
        (number "G6")
      )
      (pin power_in line (at 15.24 -2.54 180.0) (length 5.08) hide
        (name "VSS")
        (number "G7")
      )
      (pin power_in line (at 15.24 -2.54 180.0) (length 5.08) hide
        (name "VSS")
        (number "G8")
      )
      (pin power_in line (at 15.24 -2.54 180.0) (length 5.08) hide
        (name "VSS")
        (number "K10")
      )
      (pin power_in line (at 15.24 -5.08 180.0) (length 5.08)
        (name "VSS_PA")
        (number "C1")
      )
      (pin power_in line (at -15.24 -5.08 0) (length 5.08)
        (name "DEC5")
        (number "F2")
      )
      (pin power_in line (at 15.24 5.08 180.0) (length 5.08)
        (name "VDDH")
        (number "J10")
      )
      (pin power_in line (at -15.24 5.08 0) (length 5.08)
        (name "DCCH")
        (number "H9")
      )
      (pin power_in line (at -15.24 7.62 0) (length 5.08)
        (name "DECUSB")
        (number "K9")
      )
      (pin power_in line (at 15.24 10.16 180.0) (length 5.08)
        (name "VBUS")
        (number "J9")
      )
    )
    (symbol "NRF52840-CKAA-R7_3_0"
      (pin input line (at 15.24 -2.54 180.0) (length 5.08)
        (name "XC2")
        (number "A2")
      )
      (pin input line (at 15.24 0.0 180.0) (length 5.08)
        (name "XC1")
        (number "A1")
      )
      (pin input clock (at -15.24 0.0 0) (length 5.08)
        (name "SWDCLK")
        (number "H2")
      )
      (pin bidirectional line (at -15.24 -2.54 0) (length 5.08)
        (name "SWDIO")
        (number "J2")
      )
    )
  )
)