(kicad_symbol_lib (version 20211014) (generator adom-lbr)
(symbol "BLM15AG601SN1D"
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(offset 0)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "FB"
				(at -3.81 0.635 90)
			)
			(property "Value" "BLM15AG601SN1D"
				(at 3.81 0 90)
			)
			(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
				(at -1.778 0 90)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "600Ω@100MHz Ferrite Bead, 520mΩ DCR, 0402"
				(at 0 0 0)
			)
			(property "LCSC PN" "C76884"
				(at 0 0 0)
			)
			(property "ki_keywords" "L ferrite bead inductor filter"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "Inductor_* L_* *Ferrite*"
				(at 0 0 0)
			)
			(symbol "BLM15AG601SN1D_0_1")
			(symbol "BLM15AG601SN1D_1_1"
				(pin passive line
					(at 0 3.81 270)
					(length 2.54)
					(name "~")
					(number "1")
				)
				(pin passive line
					(at 0 -3.81 90)
					(length 2.54)
					(name "~")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
(symbol "C_100nF_0402"
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(offset 0.254)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "C"
				(at 0.635 2.54 0)
			)
			(property "Value" "C_100nF_0402"
				(at 0.635 -2.54 0)
			)
			(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
				(at 0.9652 -3.81 0)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "100nF 16V X7R 0402"
				(at 0 0 0)
			)
			(property "LCSC PN" "C1525"
				(at 0 0 0)
			)
			(property "ki_keywords" "cap capacitor"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "C_*"
				(at 0 0 0)
			)
			(symbol "C_100nF_0402_0_1")
			(symbol "C_100nF_0402_1_1"
				(pin passive line
					(at 0 3.81 270)
					(length 2.794)
					(name "~")
					(number "1")
				)
				(pin passive line
					(at 0 -3.81 90)
					(length 2.794)
					(name "~")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
(symbol "C_10nF_0402"
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(offset 0.254)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "C"
				(at 0.635 2.54 0)
			)
			(property "Value" "C_10nF_0402"
				(at 0.635 -2.54 0)
			)
			(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
				(at 0.9652 -3.81 0)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "10nF 50V X7R 0402"
				(at 0 0 0)
			)
			(property "LCSC PN" "C1524"
				(at 0 0 0)
			)
			(property "ki_keywords" "cap capacitor"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "C_*"
				(at 0 0 0)
			)
			(symbol "C_10nF_0402_0_1")
			(symbol "C_10nF_0402_1_1"
				(pin passive line
					(at 0 3.81 270)
					(length 2.794)
					(name "~")
					(number "1")
				)
				(pin passive line
					(at 0 -3.81 90)
					(length 2.794)
					(name "~")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
(symbol "C_10uF_0402"
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(offset 0.254)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "C"
				(at 0.635 2.54 0)
			)
			(property "Value" "C_10uF_0402"
				(at 0.635 -2.54 0)
			)
			(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
				(at 0.9652 -3.81 0)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "10uF 6.3V X5R 0402"
				(at 0 0 0)
			)
			(property "LCSC PN" "C15525"
				(at 0 0 0)
			)
			(property "ki_keywords" "cap capacitor"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "C_*"
				(at 0 0 0)
			)
			(symbol "C_10uF_0402_0_1")
			(symbol "C_10uF_0402_1_1"
				(pin passive line
					(at 0 3.81 270)
					(length 2.794)
					(name "~")
					(number "1")
				)
				(pin passive line
					(at 0 -3.81 90)
					(length 2.794)
					(name "~")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
(symbol "C_10uF_0603"
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(offset 0.254)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "C"
				(at 0.635 2.54 0)
			)
			(property "Value" "C_10uF_0603"
				(at 0.635 -2.54 0)
			)
			(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
				(at 0.9652 -3.81 0)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "10uF 10V X5R 0603"
				(at 0 0 0)
			)
			(property "LCSC PN" "C19702"
				(at 0 0 0)
			)
			(property "ki_keywords" "cap capacitor"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "C_*"
				(at 0 0 0)
			)
			(symbol "C_10uF_0603_0_1")
			(symbol "C_10uF_0603_1_1"
				(pin passive line
					(at 0 3.81 270)
					(length 2.794)
					(name "~")
					(number "1")
				)
				(pin passive line
					(at 0 -3.81 90)
					(length 2.794)
					(name "~")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
(symbol "C_18pF_0402"
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(offset 0.254)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "C"
				(at 0.635 2.54 0)
			)
			(property "Value" "C_18pF_0402"
				(at 0.635 -2.54 0)
			)
			(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
				(at 0.9652 -3.81 0)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "18pF 50V C0G 0402 Crystal Load Capacitor"
				(at 0 0 0)
			)
			(property "LCSC PN" "C1549"
				(at 0 0 0)
			)
			(property "ki_keywords" "cap capacitor"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "C_*"
				(at 0 0 0)
			)
			(symbol "C_18pF_0402_0_1")
			(symbol "C_18pF_0402_1_1"
				(pin passive line
					(at 0 3.81 270)
					(length 2.794)
					(name "~")
					(number "1")
				)
				(pin passive line
					(at 0 -3.81 90)
					(length 2.794)
					(name "~")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
(symbol "C_1uF_0402"
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(offset 0.254)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "C"
				(at 0.635 2.54 0)
			)
			(property "Value" "C_1uF_0402"
				(at 0.635 -2.54 0)
			)
			(property "Footprint" "Capacitor_SMD:C_0402_1005Metric"
				(at 0.9652 -3.81 0)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "1uF 25V X5R 0402"
				(at 0 0 0)
			)
			(property "LCSC PN" "C52923"
				(at 0 0 0)
			)
			(property "ki_keywords" "cap capacitor"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "C_*"
				(at 0 0 0)
			)
			(symbol "C_1uF_0402_0_1")
			(symbol "C_1uF_0402_1_1"
				(pin passive line
					(at 0 3.81 270)
					(length 2.794)
					(name "~")
					(number "1")
				)
				(pin passive line
					(at 0 -3.81 90)
					(length 2.794)
					(name "~")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
(symbol "HC-RJ45-511Q-1-2"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "J"
				(at 0 17.78 0)
			)
			(property "Value" "HC-RJ45-511Q-1-2"
				(at 0 -17.78 0)
			)
			(property "Footprint" "HCTL_BLT:RJ45-SMD_HC-RJ45-511Q-1-2"
				(at 0 -20.32 0)
			)
			(property "Datasheet" "https://www.lcsc.com/datasheet/C42376615.pdf"
				(at 0 -22.86 0)
			)
			(property "Description" "HCTL HC-RJ45-511Q-1-2, Vertical RJ45 8P8C Jack, Shielded, With LED and Integrated Magnetics, SMD"
				(at 0 0 0)
			)
			(property "Manufacturer" "HCTL(华灿天禄)"
				(at 0 -25.4 0)
			)
			(property "MPN" "HC-RJ45-511Q-1-2"
				(at 0 -27.94 0)
			)
			(property "LCSC PN" "C42376615"
				(at 0 -30.48 0)
			)
			(symbol "HC-RJ45-511Q-1-2_0_1"
				(pin unspecified line
					(at -17.78 5.08 0)
					(length 5.08)
					(name "LED_R+")
					(number "12")
				)
				(pin unspecified line
					(at -17.78 2.54 0)
					(length 5.08)
					(name "LED_R-")
					(number "11")
				)
				(pin unspecified line
					(at 17.78 5.08 180)
					(length 5.08)
					(name "LED_L+")
					(number "14")
				)
				(pin unspecified line
					(at 17.78 2.54 180)
					(length 5.08)
					(name "LED_L-")
					(number "13")
				)
			)
			(symbol "HC-RJ45-511Q-1-2_1_1"
				(pin unspecified line
					(at -11.43 -12.7 90)
					(length 5.08)
					(name "TD4-")
					(number "10")
				)
				(pin unspecified line
					(at -8.89 -12.7 90)
					(length 5.08)
					(name "TD4+")
					(number "9")
				)
				(pin unspecified line
					(at -6.35 -12.7 90)
					(length 5.08)
					(name "TD3-")
					(number "8")
				)
				(pin unspecified line
					(at -3.81 -12.7 90)
					(length 5.08)
					(name "TD3+")
					(number "7")
				)
				(pin unspecified line
					(at -1.27 -12.7 90)
					(length 5.08)
					(name "SHIELD")
					(number "6")
				)
				(pin unspecified line
					(at 0 12.7 270)
					(length 2.54)
					(name "SHIELD")
					(number "15")
				)
				(pin unspecified line
					(at 1.27 -12.7 90)
					(length 5.08)
					(name "SHIELD")
					(number "5")
				)
				(pin unspecified line
					(at 3.81 -12.7 90)
					(length 5.08)
					(name "TD2-")
					(number "4")
				)
				(pin unspecified line
					(at 6.35 -12.7 90)
					(length 5.08)
					(name "TD2+")
					(number "3")
				)
				(pin unspecified line
					(at 8.89 -12.7 90)
					(length 5.08)
					(name "TD1-")
					(number "2")
				)
				(pin unspecified line
					(at 11.43 -12.7 90)
					(length 5.08)
					(name "TD1+")
					(number "1")
				)
			)
			(embedded_fonts no)
		)
(symbol "HD3SS3212IRKSR"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "U"
				(at 0 17.78 0)
			)
			(property "Value" "HD3SS3212IRKSR"
				(at 0 -17.78 0)
			)
			(property "Footprint" "TI_BLT:DHVQFN-20_L4.5-W2.5-P0.50-BL-EP"
				(at 0 -20.32 0)
			)
			(property "Datasheet" "https://www.ti.com/lit/ds/symlink/hd3ss3212.pdf"
				(at 0 -22.86 0)
			)
			(property "Description" "USB 3.1 Gen1 SuperSpeed 2:1 Mux/DeMux Switch, DHVQFN-20"
				(at 0 0 0)
			)
			(property "LCSC PN" "C544517"
				(at 0 0 0)
			)
			(property "ki_keywords" "USB3.1 mux demux switch superspeed"
				(at 0 0 0)
			)
			(symbol "HD3SS3212IRKSR_0_1"
				(pin passive line
					(at -11.43 10.16 0)
					(length 2.54)
					(name "RSVD1")
					(number "1")
				)
				(pin input line
					(at -11.43 7.62 0)
					(length 2.54)
					(name "~{OE}")
					(number "2")
				)
				(pin passive line
					(at -11.43 5.08 0)
					(length 2.54)
					(name "A0P")
					(number "3")
				)
				(pin passive line
					(at -11.43 2.54 0)
					(length 2.54)
					(name "A0N")
					(number "4")
				)
				(pin power_in line
					(at -11.43 0 0)
					(length 2.54)
					(name "GND")
					(number "5")
				)
				(pin power_in line
					(at -11.43 -2.54 0)
					(length 2.54)
					(name "VCC")
					(number "6")
				)
				(pin passive line
					(at -11.43 -5.08 0)
					(length 2.54)
					(name "A1P")
					(number "7")
				)
				(pin passive line
					(at -11.43 -7.62 0)
					(length 2.54)
					(name "A1N")
					(number "8")
				)
				(pin input line
					(at -11.43 -10.16 0)
					(length 2.54)
					(name "SEL")
					(number "9")
				)
				(pin passive line
					(at -11.43 -12.7 0)
					(length 2.54)
					(name "RSVD2")
					(number "10")
				)
				(pin power_in line
					(at 11.43 12.7 180)
					(length 2.54)
					(name "EP")
					(number "21")
				)
				(pin power_in line
					(at 11.43 10.16 180)
					(length 2.54)
					(name "GND")
					(number "20")
				)
				(pin passive line
					(at 11.43 7.62 180)
					(length 2.54)
					(name "B0P")
					(number "19")
				)
				(pin passive line
					(at 11.43 5.08 180)
					(length 2.54)
					(name "B0N")
					(number "18")
				)
				(pin passive line
					(at 11.43 2.54 180)
					(length 2.54)
					(name "B1P")
					(number "17")
				)
				(pin passive line
					(at 11.43 0 180)
					(length 2.54)
					(name "B1N")
					(number "16")
				)
				(pin passive line
					(at 11.43 -2.54 180)
					(length 2.54)
					(name "C0P")
					(number "15")
				)
				(pin passive line
					(at 11.43 -5.08 180)
					(length 2.54)
					(name "C0N")
					(number "14")
				)
				(pin passive line
					(at 11.43 -7.62 180)
					(length 2.54)
					(name "C1P")
					(number "13")
				)
				(pin passive line
					(at 11.43 -10.16 180)
					(length 2.54)
					(name "C1N")
					(number "12")
				)
				(pin power_in line
					(at 11.43 -12.7 180)
					(length 2.54)
					(name "GND")
					(number "11")
				)
			)
			(embedded_fonts no)
		)
(symbol "LAN7800-I_Y9X"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "U"
				(at 0 35.56 0)
			)
			(property "Value" "LAN7800-I/Y9X"
				(at 0 -35.56 0)
			)
			(property "Footprint" "Microchip_BLT:QFN-48_L7.0-W7.0-P0.50-BL-EP5.3"
				(at 0 -38.1 0)
			)
			(property "Datasheet" "https://www.lcsc.com/datasheet/C633488.pdf"
				(at 0 -40.64 0)
			)
			(property "Description" "Microchip LAN7800 SuperSpeed USB 3.1 Gen1 to 10/100/1000 Ethernet Controller, QFN-48"
				(at 0 0 0)
			)
			(property "Manufacturer" "MICROCHIP(美国微芯)"
				(at 0 -43.18 0)
			)
			(property "LCSC PN" "C633488"
				(at 0 -48.26 0)
			)
			(property "ki_keywords" "Pre-ordered MCUs"
				(at 0 0 0)
			)
			(symbol "LAN7800-I_Y9X_0_1"
				(pin unspecified line
					(at -36.83 27.94 0)
					(length 2.54)
					(name "TR0P")
					(number "1")
				)
				(pin unspecified line
					(at -36.83 25.4 0)
					(length 2.54)
					(name "TR0N")
					(number "2")
				)
				(pin unspecified line
					(at -36.83 22.86 0)
					(length 2.54)
					(name "VDD25A")
					(number "3")
				)
				(pin unspecified line
					(at -36.83 20.32 0)
					(length 2.54)
					(name "TR1P")
					(number "4")
				)
				(pin unspecified line
					(at -36.83 17.78 0)
					(length 2.54)
					(name "TR1N")
					(number "5")
				)
				(pin unspecified line
					(at -36.83 15.24 0)
					(length 2.54)
					(name "VDD25A")
					(number "6")
				)
				(pin unspecified line
					(at -36.83 12.7 0)
					(length 2.54)
					(name "TR2P")
					(number "7")
				)
				(pin unspecified line
					(at -36.83 10.16 0)
					(length 2.54)
					(name "TR2N")
					(number "8")
				)
				(pin unspecified line
					(at -36.83 7.62 0)
					(length 2.54)
					(name "VDD25A")
					(number "9")
				)
				(pin unspecified line
					(at -36.83 5.08 0)
					(length 2.54)
					(name "TR3P")
					(number "10")
				)
				(pin unspecified line
					(at -36.83 2.54 0)
					(length 2.54)
					(name "TR3N")
					(number "11")
				)
				(pin unspecified line
					(at -36.83 0 0)
					(length 2.54)
					(name "VDD25A")
					(number "12")
				)
				(pin unspecified line
					(at -36.83 -2.54 0)
					(length 2.54)
					(name "VDD12_SW_OUT")
					(number "13")
				)
				(pin unspecified line
					(at -36.83 -5.08 0)
					(length 2.54)
					(name "VDD_SW_IN")
					(number "14")
				)
				(pin unspecified line
					(at -36.83 -7.62 0)
					(length 2.54)
					(name "VDD12_SW_FB")
					(number "15")
				)
				(pin unspecified line
					(at -36.83 -10.16 0)
					(length 2.54)
					(name "EECS/GPIO0")
					(number "16")
				)
				(pin unspecified line
					(at -36.83 -12.7 0)
					(length 2.54)
					(name "EEDI/GPIO1")
					(number "17")
				)
				(pin unspecified line
					(at -36.83 -15.24 0)
					(length 2.54)
					(name "EEDO/LED0/GPIO2")
					(number "18")
				)
				(pin unspecified line
					(at -36.83 -17.78 0)
					(length 2.54)
					(name "EECLK/LED1/GPIO3")
					(number "19")
				)
				(pin unspecified line
					(at -36.83 -20.32 0)
					(length 2.54)
					(name "VDDVARIO")
					(number "20")
				)
				(pin unspecified line
					(at -36.83 -22.86 0)
					(length 2.54)
					(name "VDD12CORE")
					(number "21")
				)
				(pin unspecified line
					(at -36.83 -25.4 0)
					(length 2.54)
					(name "PME_N/GPIO4")
					(number "22")
				)
				(pin unspecified line
					(at -36.83 -27.94 0)
					(length 2.54)
					(name "VBUS_DET")
					(number "23")
				)
				(pin unspecified line
					(at -36.83 -30.48 0)
					(length 2.54)
					(name "SUSPEND_N/LED2/GPIO5")
					(number "24")
				)
				(pin unspecified line
					(at 36.83 30.48 180)
					(length 2.54)
					(name "VSS")
					(number "49")
				)
				(pin unspecified line
					(at 36.83 27.94 180)
					(length 2.54)
					(name "REF_FILT")
					(number "48")
				)
				(pin unspecified line
					(at 36.83 25.4 180)
					(length 2.54)
					(name "REF_REXT")
					(number "47")
				)
				(pin unspecified line
					(at 36.83 22.86 180)
					(length 2.54)
					(name "VDD33_REG_IN")
					(number "46")
				)
				(pin unspecified line
					(at 36.83 20.32 180)
					(length 2.54)
					(name "VDD25_REG_OUT")
					(number "45")
				)
				(pin unspecified line
					(at 36.83 17.78 180)
					(length 2.54)
					(name "VDD12A")
					(number "44")
				)
				(pin unspecified line
					(at 36.83 15.24 180)
					(length 2.54)
					(name "PME_MODE/GPIO7")
					(number "43")
				)
				(pin unspecified line
					(at 36.83 12.7 180)
					(length 2.54)
					(name "VDD12CORE")
					(number "42")
				)
				(pin unspecified line
					(at 36.83 10.16 180)
					(length 2.54)
					(name "XO")
					(number "41")
				)
				(pin unspecified line
					(at 36.83 7.62 180)
					(length 2.54)
					(name "XI")
					(number "40")
				)
				(pin unspecified line
					(at 36.83 5.08 180)
					(length 2.54)
					(name "VDDVARIO")
					(number "39")
				)
				(pin unspecified line
					(at 36.83 2.54 180)
					(length 2.54)
					(name "VDD33A")
					(number "38")
				)
				(pin unspecified line
					(at 36.83 0 180)
					(length 2.54)
					(name "USBRBIAS")
					(number "37")
				)
				(pin unspecified line
					(at 36.83 -2.54 180)
					(length 2.54)
					(name "VDDVARIO")
					(number "36")
				)
				(pin unspecified line
					(at 36.83 -5.08 180)
					(length 2.54)
					(name "RESET_N/PME_CLEAR")
					(number "35")
				)
				(pin unspecified line
					(at 36.83 -7.62 180)
					(length 2.54)
					(name "TEST")
					(number "34")
				)
				(pin unspecified line
					(at 36.83 -10.16 180)
					(length 2.54)
					(name "LED3/GPIO6")
					(number "33")
				)
				(pin unspecified line
					(at 36.83 -12.7 180)
					(length 2.54)
					(name "USB3_RXDM")
					(number "32")
				)
				(pin unspecified line
					(at 36.83 -15.24 180)
					(length 2.54)
					(name "USB3_RXDP")
					(number "31")
				)
				(pin unspecified line
					(at 36.83 -17.78 180)
					(length 2.54)
					(name "VDD12A")
					(number "30")
				)
				(pin unspecified line
					(at 36.83 -20.32 180)
					(length 2.54)
					(name "USB3_TXDM")
					(number "29")
				)
				(pin unspecified line
					(at 36.83 -22.86 180)
					(length 2.54)
					(name "USB3_TXDP")
					(number "28")
				)
				(pin unspecified line
					(at 36.83 -25.4 180)
					(length 2.54)
					(name "USB2_DM")
					(number "27")
				)
				(pin unspecified line
					(at 36.83 -27.94 180)
					(length 2.54)
					(name "USB2_DP")
					(number "26")
				)
				(pin unspecified line
					(at 36.83 -30.48 180)
					(length 2.54)
					(name "VDD12A")
					(number "25")
				)
			)
			(embedded_fonts no)
		)
(symbol "LED_BLUE_0603"
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(offset 1.016)
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "D"
				(at 0 2.54 0)
			)
			(property "Value" "LED_BLUE_0603"
				(at 0 -2.54 0)
			)
			(property "Footprint" "LED_SMD:LED_0603_1608Metric"
				(at 0 0 0)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "Light emitting diode"
				(at 0 0 0)
			)
			(property "Sim.Pins" "1=K 2=A"
				(at 0 0 0)
			)
			(property "LCSC PN" "C2288"
				(at 0 0 0)
			)
			(property "ki_keywords" "LED diode"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "LED* LED_SMD:* LED_THT:*"
				(at 0 0 0)
			)
			(symbol "LED_BLUE_0603_0_1")
			(symbol "LED_BLUE_0603_1_1"
				(pin passive line
					(at -3.81 0 0)
					(length 2.54)
					(name "K")
					(number "1")
				)
				(pin passive line
					(at 3.81 0 180)
					(length 2.54)
					(name "A")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
(symbol "LED_RED_0603"
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(offset 1.016)
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "D"
				(at 0 2.54 0)
			)
			(property "Value" "LED_RED_0603"
				(at 0 -2.54 0)
			)
			(property "Footprint" "LED_SMD:LED_0603_1608Metric"
				(at 0 0 0)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "Light emitting diode"
				(at 0 0 0)
			)
			(property "Sim.Pins" "1=K 2=A"
				(at 0 0 0)
			)
			(property "LCSC PN" "C2286"
				(at 0 0 0)
			)
			(property "ki_keywords" "LED diode"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "LED* LED_SMD:* LED_THT:*"
				(at 0 0 0)
			)
			(symbol "LED_RED_0603_0_1")
			(symbol "LED_RED_0603_1_1"
				(pin passive line
					(at -3.81 0 0)
					(length 2.54)
					(name "K")
					(number "1")
				)
				(pin passive line
					(at 3.81 0 180)
					(length 2.54)
					(name "A")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
(symbol "LMV331IDBVR"
			(pin_names
				(offset 0.254)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "U"
				(at -6.35 6.35 0)
			)
			(property "Value" "LMV331IDBVR"
				(at 0 6.35 0)
			)
			(property "Footprint" "TI_BLT:LMV331IDBVR"
				(at 0 0 0)
			)
			(property "Datasheet" "https://www.ti.com/lit/ds/symlink/lmv331.pdf"
				(at 0 0 0)
			)
			(property "Description" "Single 2.7V-5V Push-Pull Comparator, SOT-23-5"
				(at 0 0 0)
			)
			(property "LCSC PN" "C371938"
				(at 0 0 0)
			)
			(property "ki_keywords" "comparator single push-pull"
				(at 0 0 0)
			)
			(symbol "LMV331IDBVR_0_1"
				(pin power_in line
					(at -1.27 7.62 270)
					(length 3.81)
					(name "V+")
					(number "5")
				)
				(pin power_in line
					(at -1.27 -7.62 90)
					(length 3.81)
					(name "V-")
					(number "2")
				)
			)
			(symbol "LMV331IDBVR_1_1"
				(pin input line
					(at -8.89 2.54 0)
					(length 2.54)
					(name "IN+")
					(number "1")
				)
				(pin input line
					(at -8.89 -2.54 0)
					(length 2.54)
					(name "IN-")
					(number "3")
				)
				(pin output line
					(at 7.62 0 180)
					(length 2.54)
					(name "OUT")
					(number "4")
				)
			)
			(embedded_fonts no)
		)
(symbol "L_3.3uH_1.81A_104mR_3x3"
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(offset 1.016)
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "L"
				(at -1.27 0 90)
			)
			(property "Value" "L_3.3uH_1.81A_104mR_3x3"
				(at 1.905 0 90)
			)
			(property "Footprint" "Inductor_SMD_Wurth:L_Wurth_WE-LQSH-3012"
				(at 0 0 0)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "Inductor"
				(at 0 0 0)
			)
			(property "LCSC PN" "C167749"
				(at 0 0 0)
			)
			(property "ki_keywords" "inductor choke coil reactor magnetic"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "Choke_* *Coil* Inductor_* L_*"
				(at 0 0 0)
			)
			(symbol "L_3.3uH_1.81A_104mR_3x3_0_1")
			(symbol "L_3.3uH_1.81A_104mR_3x3_1_1"
				(pin passive line
					(at 0 3.81 270)
					(length 1.27)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 0 -3.81 90)
					(length 1.27)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
(symbol "M93C66"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "U"
				(at -10.16 6.35 0)
			)
			(property "Value" "M93C66"
				(at 3.81 6.35 0)
			)
			(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
				(at 0 -10.16 0)
			)
			(property "Datasheet" "https://www.lcsc.com/datasheet/lcsc_datasheet_2304140030_STMicroelectronics-M93C66-WMN6TP_C118281.pdf"
				(at 0 -12.7 0)
			)
			(property "Description" "4Kbit (512x8) Microwire serial EEPROM, 2.5-5.5V, SOIC-8. Tie ORG (pin 6) to GND for x8 organization (LAN7800 config EEPROM)."
				(at 0 0 0)
			)
			(property "LCSC PN" "C118281"
				(at 0 0 0)
			)
			(property "MPN" "M93C66-WMN6TP"
				(at 0 0 0)
			)
			(property "Manufacturer" "STMicroelectronics"
				(at 0 0 0)
			)
			(property "ki_keywords" "EEPROM Microwire 93C66 serial nonvolatile"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
				(at 0 0 0)
			)
			(symbol "M93C66_0_1")
			(symbol "M93C66_1_1"
				(pin input line
					(at -10.16 3.81 0)
					(length 2.54)
					(name "CS")
					(number "1")
				)
				(pin input line
					(at -10.16 1.27 0)
					(length 2.54)
					(name "CLK")
					(number "2")
				)
				(pin input line
					(at -10.16 -1.27 0)
					(length 2.54)
					(name "DI")
					(number "3")
				)
				(pin tri_state line
					(at -10.16 -3.81 0)
					(length 2.54)
					(name "DO")
					(number "4")
				)
				(pin power_in line
					(at 10.16 3.81 180)
					(length 2.54)
					(name "VCC")
					(number "8")
				)
				(pin no_connect line
					(at 10.16 1.27 180)
					(length 2.54)
					(name "DU")
					(number "7")
				)
				(pin input line
					(at 10.16 -1.27 180)
					(length 2.54)
					(name "ORG")
					(number "6")
				)
				(pin power_in line
					(at 10.16 -3.81 180)
					(length 2.54)
					(name "GND")
					(number "5")
				)
			)
			(embedded_fonts no)
		)
(symbol "MachinePin"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "MP"
				(at -1.27 1.524 0)
				(do_not_autoplace)
			)
			(property "Value" ""
				(at 0 0 0)
			)
			(property "Footprint" "Adom_BLT:MachinePinMediumShort"
				(at 0 -1.524 0)
				(do_not_autoplace)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "ki_fp_filters" "MachinePin*"
				(at 0 0 0)
			)
			(symbol "MachinePin_1_0")
			(symbol "MachinePin_1_1"
				(pin passive line
					(at 5.08 0 180)
					(length 2)
					(name "")
					(number "1")
				)
			)
			(embedded_fonts no)
		)
(symbol "NCP1117-3.3_SOT223"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "U"
				(at -3.81 3.175 0)
			)
			(property "Value" "NCP1117-3.3_SOT223"
				(at 0 3.175 0)
			)
			(property "Footprint" "Package_TO_SOT_SMD:SOT-223-3_TabPin2"
				(at 0 5.08 0)
			)
			(property "Datasheet" "http://www.onsemi.com/pub_link/Collateral/NCP1117-D.PDF"
				(at 2.54 -6.35 0)
			)
			(property "Description" "1A Low drop-out regulator, Fixed Output 3.3V, SOT-223"
				(at 0 0 0)
			)
			(property "LCSC PN" "C26537"
				(at 0 0 0)
			)
			(property "ki_keywords" "REGULATOR LDO 3.3V"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "SOT?223*TabPin2*"
				(at 0 0 0)
			)
			(symbol "NCP1117-3.3_SOT223_0_1")
			(symbol "NCP1117-3.3_SOT223_1_1"
				(pin power_in line
					(at -7.62 0 0)
					(length 2.54)
					(name "VI")
					(number "3")
				)
				(pin power_in line
					(at 0 -7.62 90)
					(length 2.54)
					(name "GND")
					(number "1")
				)
				(pin power_out line
					(at 7.62 0 180)
					(length 2.54)
					(name "VO")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
(symbol "R_12K_0402"
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(offset 0)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at 2.032 0 90)
			)
			(property "Value" "R_12K_0402"
				(at 0 0 90)
			)
			(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
				(at -1.778 0 90)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "12kΩ 1% 0402 62.5mW Thick Film Resistor"
				(at 0 0 0)
			)
			(property "LCSC PN" "C25752"
				(at 0 0 0)
			)
			(property "ki_keywords" "R res resistor"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "R_*"
				(at 0 0 0)
			)
			(symbol "R_12K_0402_1_1"
				(pin passive line
					(at 0 3.81 270)
					(length 1.27)
					(name "~")
					(number "1")
				)
				(pin passive line
					(at 0 -3.81 90)
					(length 1.27)
					(name "~")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
(symbol "R_1M_0402"
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(offset 0)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at 2.032 0 90)
			)
			(property "Value" "R_1M_0402"
				(at 0 0 90)
			)
			(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
				(at -1.778 0 90)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "1M Ohm 0402 1% 50V Thick Film Resistor"
				(at 0 0 0)
			)
			(property "LCSC PN" "C409676"
				(at 0 0 0)
			)
			(property "ki_keywords" "R res resistor"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "R_*"
				(at 0 0 0)
			)
			(symbol "R_1M_0402_0_1")
			(symbol "R_1M_0402_1_1"
				(pin passive line
					(at 0 3.81 270)
					(length 1.27)
					(name "~")
					(number "1")
				)
				(pin passive line
					(at 0 -3.81 90)
					(length 1.27)
					(name "~")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
(symbol "R_2.2K_0402"
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(offset 0)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at 2.032 0 90)
			)
			(property "Value" "R_2.2K_0402"
				(at 0 0 90)
			)
			(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
				(at -1.778 0 90)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "Resistor"
				(at 0 0 0)
			)
			(property "LCSC PN" "C25879"
				(at 0 0 0)
			)
			(property "ki_keywords" "R res resistor"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "R_*"
				(at 0 0 0)
			)
			(symbol "R_2.2K_0402_1_1"
				(pin passive line
					(at 0 3.81 270)
					(length 1.27)
					(name "~")
					(number "1")
				)
				(pin passive line
					(at 0 -3.81 90)
					(length 1.27)
					(name "~")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
(symbol "R_2K_0402"
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(offset 0)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at 2.032 0 90)
			)
			(property "Value" "R_2K_0402"
				(at 0 0 90)
			)
			(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
				(at -1.778 0 90)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "2kΩ 1% 0402 62.5mW Thick Film Resistor"
				(at 0 0 0)
			)
			(property "LCSC PN" "C4109"
				(at 0 0 0)
			)
			(property "ki_keywords" "R res resistor"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "R_*"
				(at 0 0 0)
			)
			(symbol "R_2K_0402_1_1"
				(pin passive line
					(at 0 3.81 270)
					(length 1.27)
					(name "~")
					(number "1")
				)
				(pin passive line
					(at 0 -3.81 90)
					(length 1.27)
					(name "~")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
(symbol "R_300R_0402"
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(offset 0)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at 2.032 0 90)
			)
			(property "Value" "R_300R_0402"
				(at 0 0 90)
			)
			(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
				(at -1.778 0 90)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "Resistor"
				(at 0 0 0)
			)
			(property "LCSC PN" "C138010"
				(at 0 0 0)
			)
			(property "ki_keywords" "R res resistor"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "R_*"
				(at 0 0 0)
			)
			(symbol "R_300R_0402_0_1")
			(symbol "R_300R_0402_1_1"
				(pin passive line
					(at 0 3.81 270)
					(length 1.27)
					(name "~")
					(number "1")
				)
				(pin passive line
					(at 0 -3.81 90)
					(length 1.27)
					(name "~")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
(symbol "R_4.3K_0402"
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(offset 0)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at 2.032 0 90)
			)
			(property "Value" "R_4.3K_0402"
				(at 0 0 90)
			)
			(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
				(at -1.778 0 90)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "Resistor"
				(at 0 0 0)
			)
			(property "LCSC PN" "C25899"
				(at 0 0 0)
			)
			(property "ki_keywords" "R res resistor"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "R_*"
				(at 0 0 0)
			)
			(symbol "R_4.3K_0402_0_1")
			(symbol "R_4.3K_0402_1_1"
				(pin passive line
					(at 0 3.81 270)
					(length 1.27)
					(name "~")
					(number "1")
				)
				(pin passive line
					(at 0 -3.81 90)
					(length 1.27)
					(name "~")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
(symbol "R_5.1K_0402"
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(offset 0)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at 2.032 0 90)
			)
			(property "Value" "R_5.1K_0402"
				(at 0 0 90)
			)
			(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
				(at -1.778 0 90)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "Resistor"
				(at 0 0 0)
			)
			(property "LCSC PN" "C25905"
				(at 0 0 0)
			)
			(property "ki_keywords" "R res resistor"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "R_*"
				(at 0 0 0)
			)
			(symbol "R_5.1K_0402_0_1")
			(symbol "R_5.1K_0402_1_1"
				(pin passive line
					(at 0 3.81 270)
					(length 1.27)
					(name "~")
					(number "1")
				)
				(pin passive line
					(at 0 -3.81 90)
					(length 1.27)
					(name "~")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
(symbol "R_7.68k_0402"
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(offset 0)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at 2.032 0 90)
			)
			(property "Value" "R_7.68k_0402"
				(at 0 0 90)
			)
			(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
				(at -1.778 0 90)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "Resistor"
				(at 0 0 0)
			)
			(property "LCSC PN" "C25919"
				(at 0 0 0)
			)
			(property "ki_keywords" "R res resistor"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "R_*"
				(at 0 0 0)
			)
			(symbol "R_7.68k_0402_0_1")
			(symbol "R_7.68k_0402_1_1"
				(pin passive line
					(at 0 3.81 270)
					(length 1.27)
					(name "~")
					(number "1")
				)
				(pin passive line
					(at 0 -3.81 90)
					(length 1.27)
					(name "~")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
(symbol "SKRPACE010"
			(pin_names
				(offset 1.016)
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "SW"
				(at 0 5.08 0)
			)
			(property "Value" "SKRPACE010"
				(at 0 -5.08 0)
			)
			(property "Footprint" "Alps_BLT:SKRPACE010"
				(at 0 -7.62 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "Tactile Switch SPST-NO 1.96N 50mA 12VDC SMD"
				(at 0 -12.7 0)
			)
			(property "LCSC" "C139797"
				(at 0 -10.16 0)
			)
			(symbol "SKRPACE010_0_1")
			(symbol "SKRPACE010_1_1"
				(pin passive line
					(at -5.08 1.27 0)
					(length 2.54)
					(name "A")
					(number "1")
				)
				(pin passive line
					(at -5.08 -1.27 0)
					(length 2.54)
					(name "A")
					(number "2")
				)
				(pin passive line
					(at 5.08 1.27 180)
					(length 2.54)
					(name "B")
					(number "3")
				)
				(pin passive line
					(at 5.08 -1.27 180)
					(length 2.54)
					(name "B")
					(number "4")
				)
			)
			(embedded_fonts no)
		)
(symbol "TestPoint"
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(offset 0.762)
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "TP"
				(at 0 6.858 0)
			)
			(property "Value" "TestPoint"
				(at 0 5.08 0)
			)
			(property "Footprint" ""
				(at 5.08 0 0)
			)
			(property "Datasheet" "~"
				(at 5.08 0 0)
			)
			(property "Description" "test point"
				(at 0 0 0)
			)
			(property "ki_keywords" "test point tp"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "Pin* Test*"
				(at 0 0 0)
			)
			(symbol "TestPoint_0_1")
			(symbol "TestPoint_1_1"
				(pin passive line
					(at 0 0 90)
					(length 2.54)
					(name "1")
					(number "1")
				)
			)
			(embedded_fonts no)
		)
(symbol "USB4115-03-C"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "J"
				(at 0 24.13 0)
			)
			(property "Value" "USB4115-03-C"
				(at 0 -25.4 0)
			)
			(property "Footprint" "GCT_BLT:USB-C-SMD_U263-241N-4BQC04"
				(at 0 -27.94 0)
			)
			(property "Datasheet" "https://www.lcsc.com/datasheet/C5250720.pdf"
				(at 0 -30.48 0)
			)
			(property "Description" "GCT USB4115-03-C, USB Type-C 24-Pin Vertical Female Receptacle, SMD"
				(at 0 0 0)
			)
			(property "Manufacturer" "GCT"
				(at 0 -33.02 0)
			)
			(property "MPN" "USB4115-03-C"
				(at 0 -35.56 0)
			)
			(property "LCSC PN" "C5250720"
				(at 0 -38.1 0)
			)
			(symbol "USB4115-03-C_0_1"
				(pin unspecified line
					(at -13.97 19.05 0)
					(length 2.54)
					(name "GND")
					(number "A1")
				)
				(pin unspecified line
					(at -13.97 11.43 0)
					(length 2.54)
					(name "VBUS")
					(number "A4")
				)
				(pin unspecified line
					(at -13.97 8.89 0)
					(length 2.54)
					(name "CC1")
					(number "A5")
				)
				(pin unspecified line
					(at -13.97 6.35 0)
					(length 2.54)
					(name "DP1")
					(number "A6")
				)
				(pin unspecified line
					(at -13.97 3.81 0)
					(length 2.54)
					(name "DN1")
					(number "A7")
				)
				(pin unspecified line
					(at -13.97 1.27 0)
					(length 2.54)
					(name "SUB1")
					(number "A8")
				)
				(pin unspecified line
					(at -13.97 -1.27 0)
					(length 2.54)
					(name "VBUS")
					(number "A9")
				)
				(pin unspecified line
					(at -13.97 -8.89 0)
					(length 2.54)
					(name "GND")
					(number "A12")
				)
				(pin unspecified line
					(at 13.97 19.05 180)
					(length 2.54)
					(name "GND")
					(number "B12")
				)
				(pin unspecified line
					(at 13.97 11.43 180)
					(length 2.54)
					(name "VBUS")
					(number "B9")
				)
				(pin unspecified line
					(at 13.97 8.89 180)
					(length 2.54)
					(name "SUB2")
					(number "B8")
				)
				(pin unspecified line
					(at 13.97 6.35 180)
					(length 2.54)
					(name "DN2")
					(number "B7")
				)
				(pin unspecified line
					(at 13.97 3.81 180)
					(length 2.54)
					(name "DP2")
					(number "B6")
				)
				(pin unspecified line
					(at 13.97 1.27 180)
					(length 2.54)
					(name "CC2")
					(number "B5")
				)
				(pin unspecified line
					(at 13.97 -1.27 180)
					(length 2.54)
					(name "VBUS")
					(number "B4")
				)
				(pin unspecified line
					(at 13.97 -8.89 180)
					(length 2.54)
					(name "EH")
					(number "B1")
				)
				(pin unspecified line
					(at 13.97 -12.7 180)
					(length 2.54)
					(name "EH")
					(number "28")
				)
				(pin unspecified line
					(at 13.97 -15.24 180)
					(length 2.54)
					(name "EH")
					(number "27")
				)
				(pin unspecified line
					(at 13.97 -17.78 180)
					(length 2.54)
					(name "EH")
					(number "26")
				)
				(pin unspecified line
					(at 13.97 -20.32 180)
					(length 2.54)
					(name "EH")
					(number "25")
				)
			)
			(symbol "USB4115-03-C_1_1"
				(pin unspecified line
					(at -13.97 16.51 0)
					(length 2.54)
					(name "SSTX1+")
					(number "A2")
				)
				(pin unspecified line
					(at -13.97 13.97 0)
					(length 2.54)
					(name "SSTX1-")
					(number "A3")
				)
				(pin unspecified line
					(at -13.97 -3.81 0)
					(length 2.54)
					(name "SSRX2-")
					(number "A10")
				)
				(pin unspecified line
					(at -13.97 -6.35 0)
					(length 2.54)
					(name "SSRX2+")
					(number "A11")
				)
				(pin unspecified line
					(at 13.97 16.51 180)
					(length 2.54)
					(name "SSRX1+")
					(number "B11")
				)
				(pin unspecified line
					(at 13.97 13.97 180)
					(length 2.54)
					(name "SSRX1-")
					(number "B10")
				)
				(pin unspecified line
					(at 13.97 -3.81 180)
					(length 2.54)
					(name "SSTX2-")
					(number "B3")
				)
				(pin unspecified line
					(at 13.97 -6.35 180)
					(length 2.54)
					(name "SSTX2+")
					(number "B2")
				)
			)
			(embedded_fonts no)
		)
(symbol "X322525MOB4SI"
			(pin_names
				(offset 1.016)
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "Y"
				(at 3.175 5.08 0)
			)
			(property "Value" "X322525MOB4SI"
				(at 3.175 3.175 0)
			)
			(property "Footprint" "Crystal:Crystal_SMD_3225-4Pin_3.2x2.5mm"
				(at 0 0 0)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "25MHz Crystal, 12pF, ±10ppm, 3.2x2.5mm, 4-pin, GND on pins 2 and 4"
				(at 0 0 0)
			)
			(property "LCSC PN" "C9006"
				(at 0 0 0)
			)
			(property "ki_keywords" "quartz ceramic resonator oscillator"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "Crystal*"
				(at 0 0 0)
			)
			(symbol "X322525MOB4SI_0_1")
			(symbol "X322525MOB4SI_1_1"
				(pin passive line
					(at -3.81 0 0)
					(length 1.27)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 0 5.08 270)
					(length 1.27)
					(name "2")
					(number "2")
				)
				(pin passive line
					(at 0 -5.08 90)
					(length 1.27)
					(name "4")
					(number "4")
				)
				(pin passive line
					(at 3.81 0 180)
					(length 1.27)
					(name "3")
					(number "3")
				)
			)
			(embedded_fonts no)
		)
(symbol "TL331LV"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(in_pos_files yes)
		(duplicate_pin_numbers_are_jumpers no)
		(property "Reference" "U2"
			(at 12.7 6.4202 0)
			(show_name no)
			(do_not_autoplace no)
		)
		(property "Value" "TL331LV"
			(at 12.7 3.8802 0)
			(show_name no)
			(do_not_autoplace no)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5_HandSoldering"
			(at 0 0 0)
			(show_name no)
			(do_not_autoplace no)
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(show_name no)
			(do_not_autoplace no)
			(hide yes)
		)
		(property "Description" "1.65-V to 5.5-V, low-voltage single standard comparator with Pin 4 output"
			(at 0 0 0)
			(show_name no)
			(do_not_autoplace no)
			(hide yes)
		)
		(property "LCSC PN" "C783423"
			(at 0 0 0)
			(show_name no)
			(do_not_autoplace no)
			(hide yes)
		)
		(property "ki_keywords" "comparator single push-pull"
			(at 0 0 0)
			(show_name no)
			(do_not_autoplace no)
			(hide yes)
		)
		(symbol "TL331LV_0_1"
			(pin power_in line
				(at -1.27 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "2")
			)
			(pin power_in line
				(at -1.27 7.62 270)
				(length 3.81)
				(name "V+")
				(number "5")
			)
		)
		(symbol "TL331LV_1_1"
			(pin input line
				(at -8.89 2.54 0)
				(length 2.54)
				(name "IN-")
				(number "1")
			)
			(pin input line
				(at -8.89 -2.54 0)
				(length 2.54)
				(name "IN+")
				(number "3")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "OUT")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
)
