(kicad_pcb
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(4 "In1.Cu" power)
		(6 "In2.Cu" power)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
		(41 "User.2" user)
		(43 "User.3" user)
		(45 "User.4" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(thickness 0.01)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 1"
				(type "prepreg")
				(thickness 0.1)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "In1.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 2"
				(type "core")
				(thickness 1.24)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "In2.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 3"
				(type "prepreg")
				(thickness 0.1)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(thickness 0.01)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
			)
			(copper_finish "None")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting
			(front yes)
			(back yes)
		)
		(covering
			(front no)
			(back no)
		)
		(plugging
			(front no)
			(back no)
		)
		(capping no)
		(filling no)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12)
			(dashed_line_gap_ratio 3)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(variants
		(variant
			(name "V1.2")
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 61.465 57.453749 90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C6"
			(at 0 -1.16 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "C_10uF_0402"
			(at 0 1.16 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "10uF 6.3V X5R 0402"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC PN" "C15525"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/USB/")
		(sheetfile "usb.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "VDDVARIO")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "F.Cu")
		(at 74.5 71.354999)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP7"
			(at 0 -1.448 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 1.55 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/Data/")
		(sheetfile "data.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1")
			)
		)
		(duplicate_pad_numbers_are_jumpers no)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask")
			(net "VDDVARIO")
			(pinfunction "1_1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Inductor_SMD_Wurth:L_Wurth_WE-LQSH-3012"
		(layer "F.Cu")
		(at 65.9 64.304999 90)
		(descr "Semi-Shielded High Saturation Power Inductor, body 3x3mm, https://www.we-online.com/catalog/en/WE-LQSH#/articles/WE-LQSH-3012")
		(tags "SMT")
		(property "Reference" "L4"
			(at 0 -2.5 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "L_3.3uH_1.81A_104mR_3x3"
			(at 0 2.5 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Inductor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC PN" "C167749"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Choke_* *Coil* Inductor_* L_*")
		(sheetname "/Data/")
		(sheetfile "data.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.175 0 90)
			(size 0.85 2.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "VDD12CORE")
			(pinfunction "1_1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.175 0 90)
			(size 0.85 2.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "Net-(U1-VDD12_SW_OUT)")
			(pinfunction "2_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Inductor_SMD_Wurth.3dshapes/L_Wurth_WE-LQSH-3012.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 85.7 49.504999 90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C9"
			(at 0 -1.16 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "C_10nF_0402"
			(at 0 1.16 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "10nF 50V X7R 0402"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC PN" "C1524"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Data/")
		(sheetfile "data.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "VDDVARIO")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 50.75 46.224999 90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C1"
			(at 0 -1.16 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "C_10uF_0402"
			(at 0 1.16 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "10uF 6.3V X5R 0402"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC PN" "C15525"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Power/")
		(sheetfile "power.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "VDDVARIO")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 66.96 57.994999 180)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C49"
			(at 0 -1.16 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "C_1uF_0402"
			(at 0 1.16 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "1uF 25V X5R 0402"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC PN" "C52923"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Data/")
		(sheetfile "data.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "VDD25A")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "F.Cu")
		(at 61.1 67.454999)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP6"
			(at 0 -1.448 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 1.55 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/USB/")
		(sheetfile "usb.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1")
			)
		)
		(duplicate_pad_numbers_are_jumpers no)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask")
			(net "SEL")
			(pinfunction "1_1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 77.78 58.194999 90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R39"
			(at 0 -1.17 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "R_2K_0402"
			(at 0 1.17 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "2kΩ 1% 0402 62.5mW Thick Film Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC PN" "C4109"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Data/")
		(sheetfile "data.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(pad "1" smd roundrect
			(at -0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "Net-(U1-REF_REXT)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "adom-kicad-footprint-library:MachinePinLargeShort"
		(layer "F.Cu")
		(at 51.7 37.704999)
		(property "Reference" "MP1"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Value" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MachinePin*")
		(sheetname "/")
		(sheetfile "USB3toEthernetDataOnly_Molecule.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1")
			)
		)
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 5.2 5.2)
			(drill 3.45)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "/home/barrett-land/Documents/KiCAD/3D/Adom/MachinePinLargeShort.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 75.85 69.604999)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R4"
			(at 0 -1.17 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "R_4.3K_0402"
			(at 0 1.17 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC PN" "C25899"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "USB3toEthernetDataOnly_Molecule.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "VDDVARIO")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "Net-(D1-A)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 62.465 57.453749 90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C7"
			(at 0 -1.16 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "C_100nF_0402"
			(at 0 1.16 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "100nF 16V X7R 0402"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC PN" "C1525"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/USB/")
		(sheetfile "usb.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "VDDVARIO")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "F.Cu")
		(at 59.5 71.754999)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP4"
			(at 0 -1.448 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 1.55 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/USB/")
		(sheetfile "usb.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1")
			)
		)
		(duplicate_pad_numbers_are_jumpers no)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask")
			(net "CC2")
			(pinfunction "1_1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 76.53 65.944999 -90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R41"
			(at 0 -1.17 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "R_12K_0402"
			(at 0 1.17 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "12kΩ 1% 0402 62.5mW Thick Film Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC PN" "C25752"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Data/")
		(sheetfile "data.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "Net-(U1-USBRBIAS)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 61.25 40.204999 -90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R2"
			(at 0 -1.17 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "R_300R_0402"
			(at 0 1.17 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC PN" "C138010"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Ethernet/")
		(sheetfile "ethernet.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "LAN7800_LED3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "Net-(J3-LED_R+)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 59.24 65.304999 180)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C4"
			(at 0 -1.16 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "C_100nF_0402"
			(at 0 1.16 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "100nF 16V X7R 0402"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC PN" "C1525"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/USB/")
		(sheetfile "usb.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "VDDVARIO")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "HCTL_BLT:RJ45-SMD_HC-RJ45-511Q-1-2"
		(layer "F.Cu")
		(at 70.39 44.824999)
		(property "Reference" "J3"
			(at 0 -12.675 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "HC-RJ45-511Q-1-2"
			(at 0 12.675 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.lcsc.com/datasheet/C42376615.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "HCTL HC-RJ45-511Q-1-2, Vertical RJ45 8P8C Jack, Shielded, With LED and Integrated Magnetics, SMD"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC Part" "C42376615"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "HCTL(华灿天禄)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "HC-RJ45-511Q-1-2"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC PN" "C42376615"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/Ethernet/")
		(sheetfile "ethernet.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "12" "11" "10" "9" "8" "7" "6" "15" "5" "4" "3" "2" "1" "14" "13")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" thru_hole circle
			(at -7 0.08)
			(size 1.6 1.6)
			(drill 1.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "" thru_hole circle
			(at 7 0.08)
			(size 1.6 1.6)
			(drill 1.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "1" smd rect
			(at 6.08 8.67)
			(size 0.85 2.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "ETH_P1+")
			(pinfunction "TD1+_1")
			(pintype "unspecified")
		)
		(pad "2" smd rect
			(at 4.73 8.67)
			(size 0.85 2.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "ETH_P1-")
			(pinfunction "TD1-_2")
			(pintype "unspecified")
		)
		(pad "3" smd rect
			(at 3.38 8.67)
			(size 0.85 2.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "ETH_P2+")
			(pinfunction "TD2+_3")
			(pintype "unspecified")
		)
		(pad "4" smd rect
			(at 2.03 8.67)
			(size 0.85 2.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "ETH_P2-")
			(pinfunction "TD2-_4")
			(pintype "unspecified")
		)
		(pad "5" smd rect
			(at 0.68 8.67)
			(size 0.85 2.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "SHIELD")
			(pinfunction "SHIELD_5")
			(pintype "unspecified")
		)
		(pad "6" smd rect
			(at -0.68 8.67)
			(size 0.85 2.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "SHIELD")
			(pinfunction "SHIELD_6")
			(pintype "unspecified")
		)
		(pad "7" smd rect
			(at -2.03 8.67)
			(size 0.85 2.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "ETH_P3+")
			(pinfunction "TD3+_7")
			(pintype "unspecified")
		)
		(pad "8" smd rect
			(at -3.38 8.67)
			(size 0.85 2.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "ETH_P3-")
			(pinfunction "TD3-_8")
			(pintype "unspecified")
		)
		(pad "9" smd rect
			(at -4.73 8.67)
			(size 0.85 2.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "ETH_P4+")
			(pinfunction "TD4+_9")
			(pintype "unspecified")
		)
		(pad "10" smd rect
			(at -6.07 8.67)
			(size 0.85 2.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "ETH_P4-")
			(pinfunction "TD4-_10")
			(pintype "unspecified")
		)
		(pad "11" smd rect
			(at 6.55 -7.87)
			(size 1.1 4.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
			(pinfunction "LED_R-_11")
			(pintype "unspecified")
		)
		(pad "12" smd rect
			(at 4.01 -7.87)
			(size 1.1 4.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "Net-(J3-LED_R+)")
			(pinfunction "LED_R+_12")
			(pintype "unspecified")
		)
		(pad "13" smd rect
			(at -4.01 -7.87)
			(size 1.1 4.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
			(pinfunction "LED_L-_13")
			(pintype "unspecified")
		)
		(pad "14" smd rect
			(at -6.55 -7.87)
			(size 1.1 4.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "Net-(J3-LED_L+)")
			(pinfunction "LED_L+_14")
			(pintype "unspecified")
		)
		(pad "15" smd rect
			(at 0 -8.67)
			(size 2.5 2.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "SHIELD")
			(pinfunction "SHIELD_15")
			(pintype "unspecified")
		)
		(embedded_fonts no)
		(model "/home/barrett-land/Documents/KiCAD/3D/HCTL/HC-RJ45-511Q-1-2.step"
			(offset
				(xyz 0 0 16.9)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 -0)
			)
		)
	)
	(footprint "GCT_BLT:USB-C-SMD_U263-241N-4BQC04"
		(layer "F.Cu")
		(at 52.76 60.704999 180)
		(property "Reference" "J2"
			(at 0 -6.75 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "USB4115-03-C"
			(at 1.44 6.945 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.lcsc.com/datasheet/C5250720.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "GCT USB4115-03-C, USB Type-C 24-Pin Vertical Female Receptacle, SMD"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC Part" "C5250720"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "GCT"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "USB4115-03-C"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC PN" "C5250720"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/USB/")
		(sheetfile "usb.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "A1" "A2" "A3" "A4" "A5" "A6" "A7" "A8" "A9" "A10" "A11" "A12"
					"B12" "B11" "B10" "B9" "B8" "B7" "B6" "B5" "B4" "B3" "B2" "B1" "28"
					"27" "26" "25"
				)
			)
		)
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" thru_hole circle
			(at 0 -3.75 180)
			(size 0.7 0.7)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "" thru_hole circle
			(at 0 3.75 180)
			(size 0.7 0.7)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "25" thru_hole circle
			(at 2.15 -2.4 180)
			(size 1.1 1.1)
			(drill 0.700024)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pinfunction "EH_25")
			(pintype "unspecified")
		)
		(pad "26" thru_hole circle
			(at 2.15 2.4 180)
			(size 1.1 1.1)
			(drill 0.700024)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pinfunction "EH_26")
			(pintype "unspecified")
		)
		(pad "27" thru_hole circle
			(at -2.15 2.4 180)
			(size 1.1 1.1)
			(drill 0.700024)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pinfunction "EH_27")
			(pintype "unspecified")
		)
		(pad "28" thru_hole circle
			(at -2.15 -2.4 180)
			(size 1.1 1.1)
			(drill 0.700024)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pinfunction "EH_28")
			(pintype "unspecified")
		)
		(pad "A1" smd rect
			(at 0.84 -2.75 180)
			(size 0.85 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
			(pinfunction "GND_A1")
			(pintype "unspecified")
		)
		(pad "A2" smd rect
			(at 0.84 -2.25 180)
			(size 0.85 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "USB3_1TX+")
			(pinfunction "SSTX1+_A2")
			(pintype "unspecified")
		)
		(pad "A3" smd rect
			(at 0.84 -1.75 180)
			(size 0.85 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "USB3_1TX-")
			(pinfunction "SSTX1-_A3")
			(pintype "unspecified")
		)
		(pad "A4" smd rect
			(at 0.84 -1.25 180)
			(size 0.85 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "+5V")
			(pinfunction "VBUS_A4")
			(pintype "unspecified")
		)
		(pad "A5" smd rect
			(at 0.84 -0.75 180)
			(size 0.85 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "CC1")
			(pinfunction "CC1_A5")
			(pintype "unspecified")
		)
		(pad "A6" smd rect
			(at 0.84 -0.25 180)
			(size 0.85 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "USB2_D+")
			(pinfunction "DP1_A6")
			(pintype "unspecified")
		)
		(pad "A7" smd rect
			(at 0.84 0.25 180)
			(size 0.85 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "USB2_D-")
			(pinfunction "DN1_A7")
			(pintype "unspecified")
		)
		(pad "A8" smd rect
			(at 0.84 0.75 180)
			(size 0.85 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "unconnected-(J2-SUB1-PadA8)")
			(pinfunction "SUB1_A8")
			(pintype "unspecified+no_connect")
		)
		(pad "A9" smd rect
			(at 0.84 1.25 180)
			(size 0.85 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "+5V")
			(pinfunction "VBUS_A9")
			(pintype "unspecified")
		)
		(pad "A10" smd rect
			(at 0.84 1.75 180)
			(size 0.85 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "USB3_2RX-")
			(pinfunction "SSRX2-_A10")
			(pintype "unspecified")
		)
		(pad "A11" smd rect
			(at 0.84 2.25 180)
			(size 0.85 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "USB3_2RX+")
			(pinfunction "SSRX2+_A11")
			(pintype "unspecified")
		)
		(pad "A12" smd rect
			(at 0.84 2.75 180)
			(size 0.85 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
			(pinfunction "GND_A12")
			(pintype "unspecified")
		)
		(pad "B1" smd rect
			(at -0.84 2.75 180)
			(size 0.85 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
			(pinfunction "EH_B1")
			(pintype "unspecified")
		)
		(pad "B2" smd rect
			(at -0.84 2.25 180)
			(size 0.85 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "USB3_2TX+")
			(pinfunction "SSTX2+_B2")
			(pintype "unspecified")
		)
		(pad "B3" smd rect
			(at -0.84 1.75 180)
			(size 0.85 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "USB3_2TX-")
			(pinfunction "SSTX2-_B3")
			(pintype "unspecified")
		)
		(pad "B4" smd rect
			(at -0.84 1.25 180)
			(size 0.85 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "+5V")
			(pinfunction "VBUS_B4")
			(pintype "unspecified")
		)
		(pad "B5" smd rect
			(at -0.84 0.75 180)
			(size 0.85 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "CC2")
			(pinfunction "CC2_B5")
			(pintype "unspecified")
		)
		(pad "B6" smd rect
			(at -0.84 0.25 180)
			(size 0.85 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "USB2_D+")
			(pinfunction "DP2_B6")
			(pintype "unspecified")
		)
		(pad "B7" smd rect
			(at -0.84 -0.25 180)
			(size 0.85 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "USB2_D-")
			(pinfunction "DN2_B7")
			(pintype "unspecified")
		)
		(pad "B8" smd rect
			(at -0.84 -0.75 180)
			(size 0.85 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "unconnected-(J2-SUB2-PadB8)")
			(pinfunction "SUB2_B8")
			(pintype "unspecified+no_connect")
		)
		(pad "B9" smd rect
			(at -0.84 -1.25 180)
			(size 0.85 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "+5V")
			(pinfunction "VBUS_B9")
			(pintype "unspecified")
		)
		(pad "B10" smd rect
			(at -0.84 -1.75 180)
			(size 0.85 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "USB3_1RX-")
			(pinfunction "SSRX1-_B10")
			(pintype "unspecified")
		)
		(pad "B11" smd rect
			(at -0.84 -2.25 180)
			(size 0.85 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "USB3_1RX+")
			(pinfunction "SSRX1+_B11")
			(pintype "unspecified")
		)
		(pad "B12" smd rect
			(at -0.84 -2.75 180)
			(size 0.85 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
			(pinfunction "GND_B12")
			(pintype "unspecified")
		)
		(embedded_fonts no)
		(model "/home/barrett-land/Documents/KiCAD/3D/GCT/USB4115-03-C.step"
			(offset
				(xyz 0 0 -0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -0 -90)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 68 66.654999 180)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "FB3"
			(at 0 -1.17 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "BLM15AG601SN1D"
			(at 0 1.17 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "600Ω@100MHz Ferrite Bead, 520mΩ DCR, 0402"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC PN" "C76884"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Inductor_* L_* *Ferrite*")
		(sheetname "/Data/")
		(sheetfile "data.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "VDD12A_1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "VDD12CORE")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 57.25 69.954999)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R5"
			(at 0 -1.17 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "R_5.1K_0402"
			(at 0 1.17 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC PN" "C25905"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/USB/")
		(sheetfile "usb.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "CC2")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_SMD:LED_0603_1608Metric"
		(layer "F.Cu")
		(at 61.05 45.454999 -90)
		(descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "D2"
			(at 0 -1.43 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LED_RED_0603"
			(at 0 1.43 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Light emitting diode"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC PN" "C2286"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "/")
		(sheetfile "USB3toEthernetDataOnly_Molecule.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.7875 0 270)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
			(pinfunction "K_1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.7875 0 270)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "Net-(D2-A)")
			(pinfunction "A_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Adom_BLT:MachinePinLargeShort"
		(layer "F.Cu")
		(at 83.7 37.704999)
		(property "Reference" "MP2"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Value" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MachinePin*")
		(sheetname "/")
		(sheetfile "USB3toEthernetDataOnly_Molecule.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1")
			)
		)
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 5.2 5.2)
			(drill 3.45)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "/home/barrett-land/Documents/KiCAD/3D/Adom/MachinePinLargeShort.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TI_BLT:DHVQFN-20_L4.5-W2.5-P0.50-BL-EP"
		(layer "F.Cu")
		(at 61.105 61.144999 90)
		(property "Reference" "U5"
			(at 0 -5.157 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "HD3SS3212IRKSR"
			(at 0 5.157 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/hd3ss3212.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "USB 3.1 Gen1 SuperSpeed 2:1 Mux/DeMux Switch, DHVQFN-20"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC Part" "C544517"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC PN" "C544517"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/USB/")
		(sheetfile "usb.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2" "3" "4" "5" "6" "7" "8" "9" "10" "21" "20" "19" "18" "17"
					"16" "15" "14" "13" "12" "11"
				)
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -2.16 0.25 90)
			(size 0.665 0.28)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "unconnected-(U5-RSVD1-Pad1)")
			(pinfunction "RSVD1_1")
			(pintype "passive+no_connect")
		)
		(pad "2" smd rect
			(at -1.75 1.16 90)
			(size 0.28 0.665)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
			(pinfunction "~{OE}_2")
			(pintype "input")
		)
		(pad "3" smd rect
			(at -1.25 1.16 90)
			(size 0.28 0.665)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "/USB/MUX_USB3_ATX+")
			(pinfunction "A0P_3")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at -0.75 1.16 90)
			(size 0.28 0.665)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "/USB/MUX_USB3_ATX-")
			(pinfunction "A0N_4")
			(pintype "passive")
		)
		(pad "5" smd rect
			(at -0.25 1.16 90)
			(size 0.28 0.665)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
			(pinfunction "GND_5")
			(pintype "power_in")
		)
		(pad "6" smd rect
			(at 0.25 1.16 90)
			(size 0.28 0.665)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "VDDVARIO")
			(pinfunction "VCC_6")
			(pintype "power_in")
		)
		(pad "7" smd rect
			(at 0.75 1.16 90)
			(size 0.28 0.665)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "MUX_USB3_RX+")
			(pinfunction "A1P_7")
			(pintype "passive")
		)
		(pad "8" smd rect
			(at 1.25 1.16 90)
			(size 0.28 0.665)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "MUX_USB3_RX-")
			(pinfunction "A1N_8")
			(pintype "passive")
		)
		(pad "9" smd rect
			(at 1.75 1.16 90)
			(size 0.28 0.665)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "SEL")
			(pinfunction "SEL_9")
			(pintype "input")
		)
		(pad "10" smd rect
			(at 2.16 0.25 90)
			(size 0.665 0.28)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "unconnected-(U5-RSVD2-Pad10)")
			(pinfunction "RSVD2_10")
			(pintype "passive+no_connect")
		)
		(pad "11" smd rect
			(at 2.16 -0.25 90)
			(size 0.665 0.28)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
			(pinfunction "GND_11")
			(pintype "power_in")
		)
		(pad "12" smd rect
			(at 1.75 -1.16 90)
			(size 0.28 0.665)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "USB3_2RX-")
			(pinfunction "C1N_12")
			(pintype "passive")
		)
		(pad "13" smd rect
			(at 1.25 -1.16 90)
			(size 0.28 0.665)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "USB3_2RX+")
			(pinfunction "C1P_13")
			(pintype "passive")
		)
		(pad "14" smd rect
			(at 0.75 -1.16 90)
			(size 0.28 0.665)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "USB3_2TX-")
			(pinfunction "C0N_14")
			(pintype "passive")
		)
		(pad "15" smd rect
			(at 0.25 -1.16 90)
			(size 0.28 0.665)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "USB3_2TX+")
			(pinfunction "C0P_15")
			(pintype "passive")
		)
		(pad "16" smd rect
			(at -0.25 -1.16 90)
			(size 0.28 0.665)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "USB3_1RX-")
			(pinfunction "B1N_16")
			(pintype "passive")
		)
		(pad "17" smd rect
			(at -0.75 -1.16 90)
			(size 0.28 0.665)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "USB3_1RX+")
			(pinfunction "B1P_17")
			(pintype "passive")
		)
		(pad "18" smd rect
			(at -1.25 -1.16 90)
			(size 0.28 0.665)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "USB3_1TX-")
			(pinfunction "B0N_18")
			(pintype "passive")
		)
		(pad "19" smd rect
			(at -1.75 -1.16 90)
			(size 0.28 0.665)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "USB3_1TX+")
			(pinfunction "B0P_19")
			(pintype "passive")
		)
		(pad "20" smd rect
			(at -2.16 -0.25 90)
			(size 0.665 0.28)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
			(pinfunction "GND_20")
			(pintype "power_in")
		)
		(pad "21" smd rect
			(at 0 0 90)
			(size 3 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
			(pinfunction "EP_21")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/WQFN-20-1EP_2.5x4.5mm_P0.5mm_EP1x2.9mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 270)
			)
		)
	)
	(footprint "Adom_BLT:MachinePinLargeShort"
		(layer "F.Cu")
		(at 51.7 69.704999)
		(property "Reference" "MP3"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Value" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MachinePin*")
		(sheetname "/")
		(sheetfile "USB3toEthernetDataOnly_Molecule.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1")
			)
		)
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 5.2 5.2)
			(drill 3.45)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "/home/barrett-land/Documents/KiCAD/3D/Adom/MachinePinLargeShort.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 79.35 58.504999 -90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "FB2"
			(at 0 -1.17 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "BLM15AG601SN1D"
			(at 0 1.17 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "600Ω@100MHz Ferrite Bead, 520mΩ DCR, 0402"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC PN" "C76884"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Inductor_* L_* *Ferrite*")
		(sheetname "/Data/")
		(sheetfile "data.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "VDD12A_3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "VDD12CORE")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "adom-kicad-footprint-library:AdomIconMedium"
		(layer "F.Cu")
		(at 83.8 44.85)
		(property "Reference" "REF**"
			(at 0 -0.5 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "AdomIconMedium"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 60.65 65.504999 90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R9"
			(at 0 -1.17 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "R_5.1K_0402"
			(at 0 1.17 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC PN" "C25905"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/USB/")
		(sheetfile "usb.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "SEL")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "VDDVARIO")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 61.05 47.954999 90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R7"
			(at 0 -1.17 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "R_7.68k_0402"
			(at 0 1.17 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC PN" "C25919"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "USB3toEthernetDataOnly_Molecule.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "Net-(D2-A)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_SMD:LED_0603_1608Metric"
		(layer "F.Cu")
		(at 78.6 69.604999 180)
		(descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "D1"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LED_BLUE_0603"
			(at 0 1.43 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Light emitting diode"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC PN" "C2288"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "/")
		(sheetfile "USB3toEthernetDataOnly_Molecule.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.7875 0 180)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
			(pinfunction "K_1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.7875 0 180)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "Net-(D1-A)")
			(pinfunction "A_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 59.75 49.754999)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C3"
			(at 0 -1.16 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "C_100nF_0402"
			(at 0 1.16 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "100nF 16V X7R 0402"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC PN" "C1525"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/USB/")
		(sheetfile "usb.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Microchip_BLT:QFN-48_L7.0-W7.0-P0.50-BL-EP5.3"
		(layer "F.Cu")
		(at 71.88 62.019999 180)
		(property "Reference" "U1"
			(at 0 -7.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LAN7800-I/Y9X"
			(at 0 7.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.lcsc.com/datasheet/C633488.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Microchip LAN7800 SuperSpeed USB 3.1 Gen1 to 10/100/1000 Ethernet Controller, QFN-48"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC Part" "C633488"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "MICROCHIP(美国微芯)"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "LAN7800-I/Y9X"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC PN" "C633488"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/Data/")
		(sheetfile "data.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2" "3" "4" "5" "6" "7" "8" "9" "10" "11" "12" "13" "14" "15"
					"16" "17" "18" "19" "20" "21" "22" "23" "24" "49" "48" "47" "46" "45"
					"44" "43" "42" "41" "40" "39" "38" "37" "36" "35" "34" "33" "32" "31"
					"30" "29" "28" "27" "26" "25"
				)
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd oval
			(at -2.75 3.5 180)
			(size 0.28 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "ETH_P1+")
			(pinfunction "TR0P_1")
			(pintype "unspecified")
		)
		(pad "2" smd oval
			(at -2.25 3.5 180)
			(size 0.28 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "ETH_P1-")
			(pinfunction "TR0N_2")
			(pintype "unspecified")
		)
		(pad "3" smd oval
			(at -1.75 3.5 180)
			(size 0.28 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "VDD25A")
			(pinfunction "VDD25A_3")
			(pintype "unspecified")
		)
		(pad "4" smd oval
			(at -1.25 3.5 180)
			(size 0.28 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "ETH_P2+")
			(pinfunction "TR1P_4")
			(pintype "unspecified")
		)
		(pad "5" smd oval
			(at -0.75 3.5 180)
			(size 0.28 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "ETH_P2-")
			(pinfunction "TR1N_5")
			(pintype "unspecified")
		)
		(pad "6" smd oval
			(at -0.25 3.5 180)
			(size 0.28 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "VDD25A")
			(pinfunction "VDD25A_6")
			(pintype "unspecified")
		)
		(pad "7" smd oval
			(at 0.25 3.5 180)
			(size 0.28 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "ETH_P3+")
			(pinfunction "TR2P_7")
			(pintype "unspecified")
		)
		(pad "8" smd oval
			(at 0.75 3.5 180)
			(size 0.28 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "ETH_P3-")
			(pinfunction "TR2N_8")
			(pintype "unspecified")
		)
		(pad "9" smd oval
			(at 1.25 3.5 180)
			(size 0.28 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "VDD25A")
			(pinfunction "VDD25A_9")
			(pintype "unspecified")
		)
		(pad "10" smd oval
			(at 1.75 3.5 180)
			(size 0.28 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "ETH_P4+")
			(pinfunction "TR3P_10")
			(pintype "unspecified")
		)
		(pad "11" smd oval
			(at 2.25 3.5 180)
			(size 0.28 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "ETH_P4-")
			(pinfunction "TR3N_11")
			(pintype "unspecified")
		)
		(pad "12" smd oval
			(at 2.75 3.5 180)
			(size 0.28 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "VDD25A")
			(pinfunction "VDD25A_12")
			(pintype "unspecified")
		)
		(pad "13" smd oval
			(at 3.5 2.75 180)
			(size 1 0.28)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "Net-(U1-VDD12_SW_OUT)")
			(pinfunction "VDD12_SW_OUT_13")
			(pintype "unspecified")
		)
		(pad "14" smd oval
			(at 3.5 2.25 180)
			(size 1 0.28)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "VDDVARIO")
			(pinfunction "VDD_SW_IN_14")
			(pintype "unspecified")
		)
		(pad "15" smd oval
			(at 3.5 1.75 180)
			(size 1 0.28)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "VDD12CORE")
			(pinfunction "VDD12_SW_FB_15")
			(pintype "unspecified")
		)
		(pad "16" smd oval
			(at 3.5 1.25 180)
			(size 1 0.28)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "EECS")
			(pinfunction "EECS/GPIO0_16")
			(pintype "unspecified")
		)
		(pad "17" smd oval
			(at 3.5 0.75 180)
			(size 1 0.28)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "EEDO")
			(pinfunction "EEDI/GPIO1_17")
			(pintype "unspecified")
		)
		(pad "18" smd oval
			(at 3.5 0.25 180)
			(size 1 0.28)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "EEDI")
			(pinfunction "EEDO/LED0/GPIO2_18")
			(pintype "unspecified")
		)
		(pad "19" smd oval
			(at 3.5 -0.25 180)
			(size 1 0.28)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "EECLK")
			(pinfunction "EECLK/LED1/GPIO3_19")
			(pintype "unspecified")
		)
		(pad "20" smd oval
			(at 3.5 -0.75 180)
			(size 1 0.28)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "VDDVARIO")
			(pinfunction "VDDVARIO_20")
			(pintype "unspecified")
		)
		(pad "21" smd oval
			(at 3.5 -1.25 180)
			(size 1 0.28)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "VDD12CORE")
			(pinfunction "VDD12CORE_21")
			(pintype "unspecified")
		)
		(pad "22" smd oval
			(at 3.5 -1.75 180)
			(size 1 0.28)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "unconnected-(U1-PME_N{slash}GPIO4-Pad22)")
			(pinfunction "PME_N/GPIO4_22")
			(pintype "unspecified+no_connect")
		)
		(pad "23" smd oval
			(at 3.5 -2.25 180)
			(size 1 0.28)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "VDDVARIO")
			(pinfunction "VBUS_DET_23")
			(pintype "unspecified")
		)
		(pad "24" smd oval
			(at 3.5 -2.75 180)
			(size 1 0.28)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "LAN7800_LED2")
			(pinfunction "SUSPEND_N/LED2/GPIO5_24")
			(pintype "unspecified")
		)
		(pad "25" smd oval
			(at 2.75 -3.5 180)
			(size 0.28 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "VDD12A_1")
			(pinfunction "VDD12A_25")
			(pintype "unspecified")
		)
		(pad "26" smd oval
			(at 2.25 -3.5 180)
			(size 0.28 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "USB2_D+")
			(pinfunction "USB2_DP_26")
			(pintype "unspecified")
		)
		(pad "27" smd oval
			(at 1.75 -3.5 180)
			(size 0.28 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "USB2_D-")
			(pinfunction "USB2_DM_27")
			(pintype "unspecified")
		)
		(pad "28" smd oval
			(at 1.25 -3.5 180)
			(size 0.28 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "MUX_USB3_TX+")
			(pinfunction "USB3_TXDP_28")
			(pintype "unspecified")
		)
		(pad "29" smd oval
			(at 0.75 -3.5 180)
			(size 0.28 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "MUX_USB3_TX-")
			(pinfunction "USB3_TXDM_29")
			(pintype "unspecified")
		)
		(pad "30" smd oval
			(at 0.25 -3.5 180)
			(size 0.28 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "VDD12A_2")
			(pinfunction "VDD12A_30")
			(pintype "unspecified")
		)
		(pad "31" smd oval
			(at -0.25 -3.5 180)
			(size 0.28 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "MUX_USB3_RX+")
			(pinfunction "USB3_RXDP_31")
			(pintype "unspecified")
		)
		(pad "32" smd oval
			(at -0.75 -3.5 180)
			(size 0.28 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "MUX_USB3_RX-")
			(pinfunction "USB3_RXDM_32")
			(pintype "unspecified")
		)
		(pad "33" smd oval
			(at -1.25 -3.5 180)
			(size 0.28 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "LAN7800_LED3")
			(pinfunction "LED3/GPIO6_33")
			(pintype "unspecified")
		)
		(pad "34" smd oval
			(at -1.75 -3.5 180)
			(size 0.28 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
			(pinfunction "TEST_34")
			(pintype "unspecified")
		)
		(pad "35" smd oval
			(at -2.25 -3.5 180)
			(size 0.28 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "Net-(U1-RESET_N{slash}PME_CLEAR)")
			(pinfunction "RESET_N/PME_CLEAR_35")
			(pintype "unspecified")
		)
		(pad "36" smd oval
			(at -2.75 -3.5 180)
			(size 0.28 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "VDDVARIO")
			(pinfunction "VDDVARIO_36")
			(pintype "unspecified")
		)
		(pad "37" smd oval
			(at -3.5 -2.75 180)
			(size 1 0.28)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "Net-(U1-USBRBIAS)")
			(pinfunction "USBRBIAS_37")
			(pintype "unspecified")
		)
		(pad "38" smd oval
			(at -3.5 -2.25 180)
			(size 1 0.28)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "VDDVARIO")
			(pinfunction "VDD33A_38")
			(pintype "unspecified")
		)
		(pad "39" smd oval
			(at -3.5 -1.75 180)
			(size 1 0.28)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "VDDVARIO")
			(pinfunction "VDDVARIO_39")
			(pintype "unspecified")
		)
		(pad "40" smd oval
			(at -3.5 -1.25 180)
			(size 1 0.28)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "XI")
			(pinfunction "XI_40")
			(pintype "unspecified")
		)
		(pad "41" smd oval
			(at -3.5 -0.75 180)
			(size 1 0.28)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "XO")
			(pinfunction "XO_41")
			(pintype "unspecified")
		)
		(pad "42" smd oval
			(at -3.5 -0.25 180)
			(size 1 0.28)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "VDD12CORE")
			(pinfunction "VDD12CORE_42")
			(pintype "unspecified")
		)
		(pad "43" smd oval
			(at -3.5 0.25 180)
			(size 1 0.28)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "unconnected-(U1-PME_MODE{slash}GPIO7-Pad43)")
			(pinfunction "PME_MODE/GPIO7_43")
			(pintype "unspecified+no_connect")
		)
		(pad "44" smd oval
			(at -3.5 0.75 180)
			(size 1 0.28)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "VDD12A_3")
			(pinfunction "VDD12A_44")
			(pintype "unspecified")
		)
		(pad "45" smd oval
			(at -3.5 1.25 180)
			(size 1 0.28)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "VDD25A")
			(pinfunction "VDD25_REG_OUT_45")
			(pintype "unspecified")
		)
		(pad "46" smd oval
			(at -3.5 1.75 180)
			(size 1 0.28)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "VDDVARIO")
			(pinfunction "VDD33_REG_IN_46")
			(pintype "unspecified")
		)
		(pad "47" smd oval
			(at -3.5 2.25 180)
			(size 1 0.28)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "Net-(U1-REF_REXT)")
			(pinfunction "REF_REXT_47")
			(pintype "unspecified")
		)
		(pad "48" smd oval
			(at -3.5 2.75 180)
			(size 1 0.28)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "Net-(U1-REF_FILT)")
			(pinfunction "REF_FILT_48")
			(pintype "unspecified")
		)
		(pad "49" smd rect
			(at 0 0 180)
			(size 5.3 5.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
			(pinfunction "VSS_49")
			(pintype "unspecified")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/VQFN-48-1EP_7x7mm_P0.5mm_EP4.1x4.1mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 -90)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 59.35 53.054999 -90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C2"
			(at 0 -1.16 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "C_10uF_0402"
			(at 0 1.16 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "10uF 6.3V X5R 0402"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC PN" "C15525"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Power/")
		(sheetfile "power.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "+5V")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 74.30875 68.884999 90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C50"
			(at 0 -1.16 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "C_10uF_0402"
			(at 0 1.16 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "10uF 6.3V X5R 0402"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC PN" "C15525"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Data/")
		(sheetfile "data.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "VDD12CORE")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 80.625 60.725 180)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C47"
			(at 0 -1.16 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "C_18pF_0402"
			(at 0 1.16 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "18pF 50V C0G 0402 Crystal Load Capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC PN" "C1549"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Data/")
		(sheetfile "data.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "XO")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 76.53 58.174999 90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C46"
			(at 0 -1.16 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "C_1uF_0402"
			(at 0 1.16 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "1uF 25V X5R 0402"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC PN" "C52923"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Data/")
		(sheetfile "data.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(pad "1" smd roundrect
			(at -0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "Net-(U1-REF_FILT)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 67.95 67.604999)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "FB1"
			(at 0 -1.17 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "BLM15AG601SN1D"
			(at 0 1.17 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "600Ω@100MHz Ferrite Bead, 520mΩ DCR, 0402"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC PN" "C76884"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Inductor_* L_* *Ferrite*")
		(sheetname "/Data/")
		(sheetfile "data.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "VDD12CORE")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "VDD12A_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "F.Cu")
		(at 49.8 53.504999)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP3"
			(at 0 -1.448 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 1.55 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/USB/")
		(sheetfile "usb.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1")
			)
		)
		(duplicate_pad_numbers_are_jumpers no)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask")
			(net "+5V")
			(pinfunction "1_1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 78.525 65.225 180)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C48"
			(at 0 -1.16 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "C_18pF_0402"
			(at 0 1.16 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "18pF 50V C0G 0402 Crystal Load Capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC PN" "C1549"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Data/")
		(sheetfile "data.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "XI")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-223-3_TabPin2"
		(layer "F.Cu")
		(at 55.05 50.404999 90)
		(descr "module CMS SOT223 4 pins")
		(tags "CMS SOT")
		(property "Reference" "U3"
			(at 0 -4.5 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NCP1117-3.3_SOT223"
			(at 0 4.5 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://www.onsemi.com/pub_link/Collateral/NCP1117-D.PDF"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "1A Low drop-out regulator, Fixed Output 3.3V, SOT-223"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC PN" "C26537"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT?223*TabPin2*")
		(sheetname "/Power/")
		(sheetfile "power.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "3" "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -3.15 -2.3 90)
			(size 2 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
			(pinfunction "GND_1")
			(pintype "power_in")
		)
		(pad "2" smd roundrect
			(at -3.15 0 90)
			(size 2 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "VDDVARIO")
			(pinfunction "VO_2")
			(pintype "power_out")
		)
		(pad "2" smd roundrect
			(at 3.15 0 90)
			(size 2 3.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "VDDVARIO")
			(pinfunction "VO_2")
			(pintype "power_out")
		)
		(pad "3" smd roundrect
			(at -3.15 2.3 90)
			(size 2 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "+5V")
			(pinfunction "VI_3")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-223.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 60.515 57.453749 90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C8"
			(at 0 -1.16 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "C_10nF_0402"
			(at 0 1.16 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "10nF 50V X7R 0402"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC PN" "C1524"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/USB/")
		(sheetfile "usb.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "VDDVARIO")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 72.85 35.404999 -90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R6"
			(at 0 -1.17 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "R_1M_0402"
			(at 0 1.17 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "1M Ohm 0402 1% 50V Thick Film Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC PN" "C409676"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Ethernet/")
		(sheetfile "ethernet.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "SHIELD")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 60.75 52.479999 90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C5"
			(at 0 -1.43 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "C_10uF_0603"
			(at 0 1.43 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "10uF 10V X5R 0603"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC PN" "C19702"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/USB/")
		(sheetfile "usb.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "F.Cu")
		(at 58.35 37.454999)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP2"
			(at 0 -1.448 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 1.55 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/Ethernet/")
		(sheetfile "ethernet.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1")
			)
		)
		(duplicate_pad_numbers_are_jumpers no)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask")
			(net "Net-(J3-LED_L+)")
			(pinfunction "1_1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
		(layer "F.Cu")
		(at 83.175 53.789999)
		(descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOIC SO")
		(property "Reference" "U4"
			(at 0 -3.4 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "M93C66"
			(at 0 3.4 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.lcsc.com/datasheet/lcsc_datasheet_2304140030_STMicroelectronics-M93C66-WMN6TP_C118281.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "4Kbit (512x8) Microwire serial EEPROM, 2.5-5.5V, SOIC-8. Tie ORG (pin 6) to GND for x8 organization (LAN7800 config EEPROM)."
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC PN" "C118281"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "M93C66-WMN6TP"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "STMicroelectronics"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOIC*3.9x4.9mm*P1.27mm*")
		(sheetname "/Data/")
		(sheetfile "data.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2" "3" "4" "8" "7" "6" "5")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.475 -1.905)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "EECS")
			(pinfunction "CS_1")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -2.475 -0.635)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "EECLK")
			(pinfunction "CLK_2")
			(pintype "input")
		)
		(pad "3" smd roundrect
			(at -2.475 0.635)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "EEDI")
			(pinfunction "DI_3")
			(pintype "input")
		)
		(pad "4" smd roundrect
			(at -2.475 1.905)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "EEDO")
			(pinfunction "DO_4")
			(pintype "tri_state")
		)
		(pad "5" smd roundrect
			(at 2.475 1.905)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
			(pinfunction "GND_5")
			(pintype "power_in")
		)
		(pad "6" smd roundrect
			(at 2.475 0.635)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
			(pinfunction "ORG_6")
			(pintype "input")
		)
		(pad "7" smd roundrect
			(at 2.475 -0.635)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "unconnected-(U4-DU-Pad7)")
			(pinfunction "DU_7")
			(pintype "no_connect")
		)
		(pad "8" smd roundrect
			(at 2.475 -1.905)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "VDDVARIO")
			(pinfunction "VCC_8")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "F.Cu")
		(at 62.15 71.754999)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP5"
			(at 0 -1.448 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 1.55 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/USB/")
		(sheetfile "usb.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1")
			)
		)
		(duplicate_pad_numbers_are_jumpers no)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask")
			(net "CC1")
			(pinfunction "1_1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 70.3 68.304999 -90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C10"
			(at 0 -1.16 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "C_100nF_16V_0402"
			(at 0 1.16 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "100nF 16V X7R ceramic capacitor, 0402"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC PN" "C1525"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/USB/")
		(sheetfile "usb.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "MUX_USB3_TX+")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "/USB/MUX_USB3_ATX+")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "F.Cu")
		(at 80.2 42.304999)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP1"
			(at 0 -1.448 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 1.55 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/Ethernet/")
		(sheetfile "ethernet.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1")
			)
		)
		(duplicate_pad_numbers_are_jumpers no)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask")
			(net "Net-(J3-LED_R+)")
			(pinfunction "1_1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23-5_HandSoldering"
		(layer "F.Cu")
		(at 57.8 67.654999)
		(descr "5-pin SOT23 package")
		(tags "SOT-23-5 hand-soldering")
		(property "Reference" "U2"
			(at 0 -2.9 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TL331LV"
			(at 0 2.9 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "1.65-V to 5.5-V, low-voltage single standard comparator with Pin 4 output"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC PN" "C783423"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/USB/")
		(sheetfile "usb.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "3" "5" "2" "4")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.35 -0.95)
			(size 1.56 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "CC1")
			(pinfunction "IN-_1")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -1.35 0)
			(size 1.56 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
			(pinfunction "V-_2")
			(pintype "power_in")
		)
		(pad "3" smd roundrect
			(at -1.35 0.95)
			(size 1.56 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "CC2")
			(pinfunction "IN+_3")
			(pintype "input")
		)
		(pad "4" smd roundrect
			(at 1.35 0.95)
			(size 1.56 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "SEL")
			(pinfunction "OUT_4")
			(pintype "output")
		)
		(pad "5" smd roundrect
			(at 1.35 -0.95)
			(size 1.56 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "VDDVARIO")
			(pinfunction "V+_5")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 57.2 65.304999)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R3"
			(at 0 -1.17 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "R_5.1K_0402"
			(at 0 1.17 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC PN" "C25905"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/USB/")
		(sheetfile "usb.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "CC1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 56.6 42.904999)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R8"
			(at 0 -1.17 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "R_2.2K_0402"
			(at 0 1.17 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC PN" "C25879"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Data/")
		(sheetfile "data.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "Net-(U1-RESET_N{slash}PME_CLEAR)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "VDDVARIO")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Alps_BLT:SKRPACE010"
		(layer "F.Cu")
		(at 52.475 43.079999)
		(property "Reference" "SW1"
			(at 0 -2.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "SKRPACE010"
			(at 0 2.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Tactile Switch SPST-NO 1.96N 50mA 12VDC SMD"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC Part" "C139797"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC" "C139797"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/Data/")
		(sheetfile "data.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2" "3" "4")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.075 -1.075)
			(size 1.05 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
			(pinfunction "A_1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.075 -1.075)
			(size 1.05 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
			(pinfunction "A_2")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at -2.075 1.075)
			(size 1.05 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "Net-(U1-RESET_N{slash}PME_CLEAR)")
			(pinfunction "B_3")
			(pintype "passive")
		)
		(pad "4" smd roundrect
			(at 2.075 1.075)
			(size 1.05 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "Net-(U1-RESET_N{slash}PME_CLEAR)")
			(pinfunction "B_4")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "/home/barrett-land/Documents/KiCAD/3D/Alps/SKRPACE010.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 61.3 37.394999 90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R1"
			(at 0 -1.17 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "R_300R_0402"
			(at 0 1.17 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC PN" "C138010"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Ethernet/")
		(sheetfile "ethernet.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "LAN7800_LED2")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "Net-(J3-LED_L+)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Crystal:Crystal_SMD_3225-4Pin_3.2x2.5mm"
		(layer "F.Cu")
		(at 79.025 62.975)
		(descr "SMD3225/4, Crystal, 3.2x2.5mm package, SMD, generated with kicad-footprint-generator make_crystal.py, http://www.txccrystal.com/images/pdf/7m-accuracy.pdf")
		(property "Reference" "Y1"
			(at 0.000001 -2.45 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "X322525MOB4SI"
			(at -0.000001 2.45 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "25MHz Crystal, 12pF, ±10ppm, 3.2x2.5mm, 4-pin, GND on pins 2 and 4"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC PN" "C9006"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Crystal*")
		(sheetname "/Data/")
		(sheetfile "data.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2" "4" "3")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.100001 0.85)
			(size 1.4 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net "XI")
			(pinfunction "1_1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.1 0.85)
			(size 1.4 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net "GND")
			(pinfunction "2_2")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 1.100001 -0.85)
			(size 1.4 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net "XO")
			(pinfunction "3_3")
			(pintype "passive")
		)
		(pad "4" smd roundrect
			(at -1.1 -0.85)
			(size 1.4 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net "GND")
			(pinfunction "4_4")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Crystal.3dshapes/Crystal_SMD_3225-4Pin_3.2x2.5mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "adom-kicad-footprint-library:MachinePinLargeShort"
		(layer "F.Cu")
		(at 83.7 69.704999)
		(property "Reference" "MP4"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Value" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MachinePin*")
		(sheetname "/")
		(sheetfile "USB3toEthernetDataOnly_Molecule.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1")
			)
		)
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 5.2 5.2)
			(drill 3.45)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "/home/barrett-land/Documents/KiCAD/3D/Adom/MachinePinLargeShort.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 71.25 68.304999 -90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C11"
			(at 0 -1.16 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "C_100nF_16V_0402"
			(at 0 1.16 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "100nF 16V X7R ceramic capacitor, 0402"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC PN" "C1525"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/USB/")
		(sheetfile "usb.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "MUX_USB3_TX-")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "/USB/MUX_USB3_ATX-")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_arc
		(start 47.7 35.704999)
		(mid 48.285786 34.290785)
		(end 49.7 33.704999)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 47.7 71.704999)
		(end 47.7 35.704999)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 49.7 33.704999)
		(end 85.7 33.704999)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 49.7 73.704999)
		(mid 48.285786 73.119213)
		(end 47.7 71.704999)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 85.7 33.704999)
		(mid 87.114214 34.290785)
		(end 87.7 35.704999)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 85.7 73.704999)
		(end 49.7 73.704999)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 87.7 35.704999)
		(end 87.7 71.704999)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 87.7 71.704999)
		(mid 87.114214 73.119213)
		(end 85.7 73.704999)
		(layer "Edge.Cuts")
	)
	(gr_text "CC2"
		(at 57.15 71.7 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "CC1"
		(at 64.25 71.8 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "USB_DIR"
		(at 64.45 67.6 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "if you can read this \nsomething has\ngone very wrong"
		(at 70.6 43.525 0)
		(layer "F.SilkS")
	)
	(gr_text "3.3V"
		(at 72.3 71.45 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "3.3V"
		(at 78.6 68.104999 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "USB_VBUS"
		(at 49.55 49.554999 90)
		(layer "F.SilkS" knockout)
	)
	(gr_text "RST"
		(at 55.8 41.154999 90)
		(layer "F.SilkS" knockout)
	)
	(gr_text "LED_L+"
		(at 58.35 40.554999 90)
		(layer "F.SilkS" knockout)
	)
	(gr_text "5V"
		(at 59.65 45.554999 90)
		(layer "F.SilkS" knockout)
	)
	(gr_text "LED_R+"
		(at 80.25 45.654999 90)
		(layer "F.SilkS" knockout)
	)
	(gr_text "USB 3.0 to Ethernet Adapter\nv1.3: 07-28-26"
		(at 71.8 49.104999 0)
		(layer "B.SilkS" knockout)
	)
	(zone
		(net "GND")
		(layers "In1.Cu" "In2.Cu")
		(hatch edge 0.5)
		(priority 4)
		(connect_pads yes
			(clearance 0.127)
		)
		(min_thickness 0.25)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 0)
		)
		(polygon
			(pts
				(xy 45.1 31.754999) (xy 89.5 31.804999) (xy 89.6 74.954999) (xy 46.1 75.354999)
			)
		)
	)
	(embedded_fonts no)
)
