<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description></description>
<packages>
<package name="ADS124S08IPBSR">
  <description>ADS124S08IPBSR</description>
</package>
</packages>
<symbols>
<symbol name="ADS124S08IPBSR">
  <pin name="AINCOM" direction="io"/>
  <pin name="AIN5" direction="io"/>
  <pin name="AIN4" direction="io"/>
  <pin name="AIN3" direction="io"/>
  <pin name="AIN2" direction="io"/>
  <pin name="AIN1" direction="io"/>
  <pin name="AIN0" direction="io"/>
  <pin name="START/SYNC" direction="io"/>
  <pin name="~{CS}" direction="io"/>
  <pin name="DIN" direction="io"/>
  <pin name="SCLK" direction="io"/>
  <pin name="DOUT/~{DRDY}" direction="io"/>
  <pin name="~{DRDY}" direction="io"/>
  <pin name="DGND" direction="pwr"/>
  <pin name="IOVDD" direction="pwr"/>
  <pin name="DVDD" direction="pwr"/>
  <pin name="REFCOM" direction="io"/>
  <pin name="REFOUT" direction="io"/>
  <pin name="GPIO0/AIN8" direction="io"/>
  <pin name="GPIO1/AIN9" direction="io"/>
  <pin name="GPIO2/AIN10" direction="io"/>
  <pin name="GPIO3/AIN11" direction="io"/>
  <pin name="~{RESET}" direction="io"/>
  <pin name="CLK" direction="in"/>
  <pin name="REFP1/AIN6" direction="io"/>
  <pin name="REFN1/AIN7" direction="io"/>
  <pin name="REFP0" direction="io"/>
  <pin name="REFN0" direction="io"/>
  <pin name="AVSS-SW" direction="pwr"/>
  <pin name="AVSS" direction="pwr"/>
  <pin name="AVDD" direction="pwr"/>
  <pin name="NC" direction="io"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="ADS124S08IPBSR" prefix="IC">
  <description></description>
  <gates>
    <gate name="G$1" symbol="ADS124S08IPBSR"/>
  </gates>
  <devices>
    <device name="" package="ADS124S08IPBSR">
      <connects>
        <connect gate="G$1" pin="AINCOM" pad="1"/>
        <connect gate="G$1" pin="AIN5" pad="2"/>
        <connect gate="G$1" pin="AIN4" pad="3"/>
        <connect gate="G$1" pin="AIN3" pad="4"/>
        <connect gate="G$1" pin="AIN2" pad="5"/>
        <connect gate="G$1" pin="AIN1" pad="6"/>
        <connect gate="G$1" pin="AIN0" pad="7"/>
        <connect gate="G$1" pin="START/SYNC" pad="8"/>
        <connect gate="G$1" pin="~{CS}" pad="9"/>
        <connect gate="G$1" pin="DIN" pad="10"/>
        <connect gate="G$1" pin="SCLK" pad="11"/>
        <connect gate="G$1" pin="DOUT/~{DRDY}" pad="12"/>
        <connect gate="G$1" pin="~{DRDY}" pad="13"/>
        <connect gate="G$1" pin="DGND" pad="14"/>
        <connect gate="G$1" pin="IOVDD" pad="15"/>
        <connect gate="G$1" pin="DVDD" pad="16"/>
        <connect gate="G$1" pin="REFCOM" pad="24"/>
        <connect gate="G$1" pin="REFOUT" pad="23"/>
        <connect gate="G$1" pin="GPIO0/AIN8" pad="22"/>
        <connect gate="G$1" pin="GPIO1/AIN9" pad="21"/>
        <connect gate="G$1" pin="GPIO2/AIN10" pad="20"/>
        <connect gate="G$1" pin="GPIO3/AIN11" pad="19"/>
        <connect gate="G$1" pin="~{RESET}" pad="18"/>
        <connect gate="G$1" pin="CLK" pad="17"/>
        <connect gate="G$1" pin="REFP1/AIN6" pad="32"/>
        <connect gate="G$1" pin="REFN1/AIN7" pad="31"/>
        <connect gate="G$1" pin="REFP0" pad="30"/>
        <connect gate="G$1" pin="REFN0" pad="29"/>
        <connect gate="G$1" pin="AVSS-SW" pad="28"/>
        <connect gate="G$1" pin="AVSS" pad="27"/>
        <connect gate="G$1" pin="AVDD" pad="26"/>
        <connect gate="G$1" pin="NC" pad="25"/>
      </connects>
      <technologies><technology name=""/></technologies>
    </device>
  </devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>