<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>Diodes Incorporated AP62300T 3 A synchronous buck converter, 4.2 to 18 V input, 0.8 to 7 V output, COT control, 0.763 V feedback reference, 155 uA quiescent current with PFM at light load, 750 kHz typical, integrated 75 mOhm high-side and 45 mOhm low-side MOSFETs, 6-pin TSOT-26</description>
<packages>
<package name="AP62300TWU-7">
  <description>AP62300TWU-7</description>
</package>
</packages>
<symbols>
<symbol name="AP62300TWU-7">
  <pin name="VIN" direction="pwr"/>
  <pin name="EN" direction="in"/>
  <pin name="GND" direction="pwr"/>
  <pin name="SW" direction="out"/>
  <pin name="BST" direction="pas"/>
  <pin name="FB" direction="in"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="AP62300TWU-7" prefix="U">
  <description>Diodes Incorporated AP62300T 3 A synchronous buck converter, 4.2 to 18 V input, 0.8 to 7 V output, COT control, 0.763 V feedback reference, 155 uA quiescent current with PFM at light load, 750 kHz typical, integrated 75 mOhm high-side and 45 mOhm low-side MOSFETs, 6-pin TSOT-26</description>
  <gates>
    <gate name="G$1" symbol="AP62300TWU-7"/>
  </gates>
  <devices>
    <device name="" package="AP62300TWU-7">
      <connects>
        <connect gate="G$1" pin="VIN" pad="3"/>
        <connect gate="G$1" pin="EN" pad="5"/>
        <connect gate="G$1" pin="GND" pad="1"/>
        <connect gate="G$1" pin="SW" pad="2"/>
        <connect gate="G$1" pin="BST" pad="6"/>
        <connect gate="G$1" pin="FB" pad="4"/>
      </connects>
      <technologies><technology name=""/></technologies>
    </device>
  </devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>