<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>Texas Instruments LP5912-Q1 automotive 500 mA low-noise low-IQ LDO, fixed 1.1 V output, 1.6 to 6.5 V input, 12 uVRMS noise, 75 dB PSRR at 1 kHz, 30 uA typ IQ, power-good output, AEC-Q100 grade 1, 6-pin WSON (DRV) 2.00 x 2.00 mm</description>
<packages>
<package name="LP5912Q1.1DRVRQ1">
  <description>LP5912Q1.1DRVRQ1</description>
</package>
</packages>
<symbols>
<symbol name="LP5912Q1.1DRVRQ1">
  <pin name="IN" direction="pwr"/>
  <pin name="EN" direction="in"/>
  <pin name="NC" direction="io"/>
  <pin name="OUT" direction="out"/>
  <pin name="PG" direction="oc"/>
  <pin name="GND" direction="pwr"/>
  <pin name="EP" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="LP5912Q1.1DRVRQ1" prefix="U">
  <description>Texas Instruments LP5912-Q1 automotive 500 mA low-noise low-IQ LDO, fixed 1.1 V output, 1.6 to 6.5 V input, 12 uVRMS noise, 75 dB PSRR at 1 kHz, 30 uA typ IQ, power-good output, AEC-Q100 grade 1, 6-pin WSON (DRV) 2.00 x 2.00 mm</description>
  <gates>
    <gate name="G$1" symbol="LP5912Q1.1DRVRQ1"/>
  </gates>
  <devices>
    <device name="" package="LP5912Q1.1DRVRQ1">
      <connects>
        <connect gate="G$1" pin="IN" pad="6"/>
        <connect gate="G$1" pin="EN" pad="4"/>
        <connect gate="G$1" pin="NC" pad="2"/>
        <connect gate="G$1" pin="OUT" pad="1"/>
        <connect gate="G$1" pin="PG" pad="3"/>
        <connect gate="G$1" pin="GND" pad="5"/>
        <connect gate="G$1" pin="EP" pad="7"/>
      </connects>
      <technologies><technology name=""/></technologies>
    </device>
  </devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>