<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>Resistor</description>
<packages>
<package name="CR0402-FX-4700GLF">
  <description>CR0402-FX-4700GLF</description>
</package>
</packages>
<symbols>
<symbol name="CR0402-FX-4700GLF">
  <pin name="~" direction="pas"/>
  <pin name="~@2" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="CR0402-FX-4700GLF" prefix="R">
  <description>Resistor</description>
  <gates>
    <gate name="G$1" symbol="CR0402-FX-4700GLF"/>
  </gates>
  <devices>
    <device name="" package="CR0402-FX-4700GLF">
      <connects>
        <connect gate="G$1" pin="~" pad="1"/>
        <connect gate="G$1" pin="~@2" pad="2"/>
      </connects>
      <technologies>
        <technology name="">
          <attribute name="MPN" value="CR0402-FX-4700GLF"/>
        </technology>
      </technologies>
    </device>
  </devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>