<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>Intelligent control LED integrated light source, 2020 package. Built-in IC for single-wire addressable RGB control. 256 brightness levels, 16.7M colors.</description>
<packages>
<package name="WS2812B-2020">
  <description>WS2812B-2020</description>
</package>
</packages>
<symbols>
<symbol name="WS2812B-2020">
  <pin name="DOUT" direction="out"/>
  <pin name="DIN" direction="in"/>
  <pin name="VSS" direction="pwr"/>
  <pin name="VDD" direction="pwr"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WS2812B-2020" prefix="D">
  <description>Intelligent control LED integrated light source, 2020 package. Built-in IC for single-wire addressable RGB control. 256 brightness levels, 16.7M colors.</description>
  <gates>
    <gate name="G$1" symbol="WS2812B-2020"/>
  </gates>
  <devices>
    <device name="" package="WS2812B-2020">
      <connects>
        <connect gate="G$1" pin="DOUT" pad="2"/>
        <connect gate="G$1" pin="DIN" pad="4"/>
        <connect gate="G$1" pin="VSS" pad="3"/>
        <connect gate="G$1" pin="VDD" pad="1"/>
      </connects>
      <technologies>
        <technology name="">
          <attribute name="MF" value="Worldsemi"/>
          <attribute name="MPN" value="WS2812B-2020"/>
        </technology>
      </technologies>
    </device>
  </devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>