<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.7.0">
<drawing>
<board>
<plain>
<wire x1="147.2" y1="-1.4" x2="147.2" y2="129.4" width="0" layer="20"/>
<wire x1="147.2" y1="129.4" x2="145.4" y2="131.2" width="0" layer="20" curve="90"/>
<wire x1="145.4" y1="131.2" x2="-1.4" y2="131.2" width="0" layer="20"/>
<wire x1="-1.4" y1="131.2" x2="-3.2" y2="129.4" width="0" layer="20" curve="90"/>
<wire x1="-3.2" y1="129.4" x2="-3.2" y2="-1.6" width="0" layer="20"/>
<wire x1="-3.2" y1="-1.6" x2="-1.6" y2="-3.2" width="0" layer="20" curve="90"/>
<wire x1="-1.6" y1="-3.2" x2="145.4" y2="-3.2" width="0" layer="20"/>
<wire x1="145.4" y1="-3.2" x2="147.2" y2="-1.4" width="0" layer="20" curve="90"/>
<hole x="13.7" y="94.85" drill="3.1"/>
<hole x="129.7" y="94.85" drill="3.1"/>
<hole x="129.7" y="33.85" drill="3.1"/>
<hole x="13.7" y="33.85" drill="3.1"/>
<text>Pulse Generator - PG4</text>
<text>Pulse Generator - PG4</text>
</plain>
<libraries>
<library name="TSW-113-05-L-D">
<packages>
<package name="SAMTEC_TSW-113-05-L-D">
</package>
</packages>
</library>
<library name="Adom_Library_Master Library">
<packages>
<package name="CONTACT_MED">
</package>
<package name="MACH_PIN_LRG_STD">
</package>
<package name="3X1_COMPONENT">
</package>
<package name="3X1_JUMP">
</package>
<package name="MACH_PIN_LRG_SHORT">
</package>
</packages>
</library>
<library name="Adom JLCPCB Basic Parts Generated - Mar22_2025">
<description>Adom JLCPCB Basic Parts This library contains JLC components that have been matched to Eagle components.</description>
<packages>
<package name="LEDC2012X110N_FLAT-R">
<description>Chip LED, 2.00 X 1.25 X 1.10 mm body Chip LED package with body size 2.00 X 1.25 X 1.10 mm</description>
</package>
<package name="SODFL3718X115">
<description>SODFL, 3.70 mm span, 2.80 X 1.80 X 1.15 mm body SODFL package with 3.70 mm span with body size 2.80 X 1.80 X 1.15 mm</description>
</package>
</packages>
</library>
<library name="COSMIIC Library">
<packages>
<package name="COSMIIC+ADOM_BIG">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J1" library="TSW-113-05-L-D" package="SAMTEC_TSW-113-05-L-D" value="TSW-113-05-L-D">
<attribute name="MANUFACTURER" value="Samtec"/>
<attribute name="NAME"/>
<attribute name="PARTREV" value="R"/>
<attribute name="STANDARD" value="Manufacturer Recommendations"/>
<attribute name="VALUE"/>
</element>
<element name="MP5" library="Adom_Library_Master Library" package="CONTACT_MED" value="BUSA">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="MP6" library="Adom_Library_Master Library" package="CONTACT_MED" value="BUSB">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="MP7" library="Adom_Library_Master Library" package="CONTACT_MED" value="BUSA">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="MP8" library="Adom_Library_Master Library" package="CONTACT_MED" value="BUSB">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="MP52" library="Adom_Library_Master Library" package="CONTACT_MED" value="TISSUE">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="MP53" library="Adom_Library_Master Library" package="CONTACT_MED" value="GND">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="MP54" library="Adom_Library_Master Library" package="CONTACT_MED" value="TIS">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="MP55" library="Adom_Library_Master Library" package="CONTACT_MED" value="GND">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="MP1" library="Adom_Library_Master Library" package="MACH_PIN_LRG_SHORT" value="GND">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="MP2" library="Adom_Library_Master Library" package="MACH_PIN_LRG_SHORT" value="3V3">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="MP3" library="Adom_Library_Master Library" package="MACH_PIN_LRG_SHORT" value="3V3">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="MP4" library="Adom_Library_Master Library" package="MACH_PIN_LRG_SHORT" value="GND">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="Adom_Library_Master Library" package="3X1_COMPONENT" value="COMPONENT_3X1">
<attribute name="NAME"/>
<attribute name="P1" value="TIS"/>
<attribute name="P1" value="TIS"/>
<attribute name="P2" value="ANO"/>
<attribute name="VALUE"/>
</element>
<element name="MP60" library="Adom_Library_Master Library" package="CONTACT_MED" value="GND">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="MP61" library="Adom_Library_Master Library" package="CONTACT_MED" value="GND">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="MP64" library="Adom_Library_Master Library" package="CONTACT_MED" value="GND">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="MP65" library="Adom_Library_Master Library" package="CONTACT_MED" value="GND">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="MP66" library="Adom_Library_Master Library" package="CONTACT_MED" value="GND">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="MP67" library="Adom_Library_Master Library" package="CONTACT_MED" value="GND">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="MP68" library="Adom_Library_Master Library" package="CONTACT_MED" value="GND">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="MP69" library="Adom_Library_Master Library" package="CONTACT_MED" value="GND">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="MP51" library="Adom_Library_Master Library" package="CONTACT_MED" value="BUSA">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="MP50" library="Adom_Library_Master Library" package="CONTACT_MED" value="BUSB">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="MP49" library="Adom_Library_Master Library" package="CONTACT_MED" value="GND">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="MP48" library="Adom_Library_Master Library" package="CONTACT_MED" value="CH1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="MP47" library="Adom_Library_Master Library" package="CONTACT_MED" value="CH2">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="MP46" library="Adom_Library_Master Library" package="CONTACT_MED" value="CH3">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="MP45" library="Adom_Library_Master Library" package="CONTACT_MED" value="CH4">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="MP44" library="Adom_Library_Master Library" package="CONTACT_MED" value="GND">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="MP43" library="Adom_Library_Master Library" package="CONTACT_MED" value="3V3">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="MP42" library="Adom_Library_Master Library" package="CONTACT_MED" value="VIN">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="MP41" library="Adom_Library_Master Library" package="CONTACT_MED" value="GND">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="MP40" library="Adom_Library_Master Library" package="CONTACT_MED" value="TXCAN">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="MP39" library="Adom_Library_Master Library" package="CONTACT_MED" value="RXCAN">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="MP38" library="Adom_Library_Master Library" package="CONTACT_MED" value="GND">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="MP37" library="Adom_Library_Master Library" package="CONTACT_MED" value="nRESET">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="MP36" library="Adom_Library_Master Library" package="CONTACT_MED" value="ANODE">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="MP35" library="Adom_Library_Master Library" package="CONTACT_MED" value="GND">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="MP34" library="Adom_Library_Master Library" package="CONTACT_MED" value="SDATA">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="MP33" library="Adom_Library_Master Library" package="CONTACT_MED" value="SCLOCK">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="MP32" library="Adom_Library_Master Library" package="CONTACT_MED" value="GND">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="MP31" library="Adom_Library_Master Library" package="CONTACT_MED" value="SCK">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="MP30" library="Adom_Library_Master Library" package="CONTACT_MED" value="MOSI">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="MP29" library="Adom_Library_Master Library" package="CONTACT_MED" value="MISO">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="MP28" library="Adom_Library_Master Library" package="CONTACT_MED" value="GND">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="MP27" library="Adom_Library_Master Library" package="CONTACT_MED" value="TXD0">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="MP26" library="Adom_Library_Master Library" package="CONTACT_MED" value="RXD0">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="MP25" library="Adom_Library_Master Library" package="CONTACT_MED" value="GND">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="MP24" library="Adom_Library_Master Library" package="CONTACT_MED" value="TDI">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="MP23" library="Adom_Library_Master Library" package="CONTACT_MED" value="TDO">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="MP22" library="Adom_Library_Master Library" package="CONTACT_MED" value="TCK">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="MP21" library="Adom_Library_Master Library" package="CONTACT_MED" value="TMS">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="MP20" library="Adom_Library_Master Library" package="CONTACT_MED" value="GND">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D5" library="Adom JLCPCB Basic Parts Generated - Mar22_2025" package="LEDC2012X110N_FLAT-R" value="LED 0805 C34499">
<attribute name="CATEGORY" value="Optocouplers &amp; LEDs &amp; Infrared"/>
<attribute name="DATASHEET" value="https://www.lcsc.com/datasheet/lcsc_datasheet_2305091500_Hubei-KENTO-Elec-KT-0805W_C34499.pdf"/>
<attribute name="DESC" value="LED"/>
<attribute name="FULL_DESC" value="LED Indication - Discrete"/>
<attribute name="JLC_ROT" value="0"/>
<attribute name="LCSC" value="C34499"/>
<attribute name="MANUFACTURER" value="Hubei KENTO Elec"/>
<attribute name="MPN" value="KT-0805W"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="0805"/>
<attribute name="SOLDER_JOINTS" value="2"/>
<attribute name="SUBCATEGORY" value="Light Emitting Diodes (LED)"/>
<attribute name="VALUE"/>
</element>
<element name="D3" library="Adom JLCPCB Basic Parts Generated - Mar22_2025" package="LEDC2012X110N_FLAT-R" value="LED 0805 C34499">
<attribute name="CATEGORY" value="Optocouplers &amp; LEDs &amp; Infrared"/>
<attribute name="DATASHEET" value="https://www.lcsc.com/datasheet/lcsc_datasheet_2305091500_Hubei-KENTO-Elec-KT-0805W_C34499.pdf"/>
<attribute name="DESC" value="LED"/>
<attribute name="FULL_DESC" value="LED Indication - Discrete"/>
<attribute name="JLC_ROT" value="0"/>
<attribute name="LCSC" value="C34499"/>
<attribute name="MANUFACTURER" value="Hubei KENTO Elec"/>
<attribute name="MPN" value="KT-0805W"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="0805"/>
<attribute name="SOLDER_JOINTS" value="2"/>
<attribute name="SUBCATEGORY" value="Light Emitting Diodes (LED)"/>
<attribute name="VALUE"/>
</element>
<element name="D6" library="Adom JLCPCB Basic Parts Generated - Mar22_2025" package="LEDC2012X110N_FLAT-R" value="LED 0805 C34499">
<attribute name="CATEGORY" value="Optocouplers &amp; LEDs &amp; Infrared"/>
<attribute name="DATASHEET" value="https://www.lcsc.com/datasheet/lcsc_datasheet_2305091500_Hubei-KENTO-Elec-KT-0805W_C34499.pdf"/>
<attribute name="DESC" value="LED"/>
<attribute name="FULL_DESC" value="LED Indication - Discrete"/>
<attribute name="JLC_ROT" value="0"/>
<attribute name="LCSC" value="C34499"/>
<attribute name="MANUFACTURER" value="Hubei KENTO Elec"/>
<attribute name="MPN" value="KT-0805W"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="0805"/>
<attribute name="SOLDER_JOINTS" value="2"/>
<attribute name="SUBCATEGORY" value="Light Emitting Diodes (LED)"/>
<attribute name="VALUE"/>
</element>
<element name="D8" library="Adom JLCPCB Basic Parts Generated - Mar22_2025" package="LEDC2012X110N_FLAT-R" value="LED 0805 C34499">
<attribute name="CATEGORY" value="Optocouplers &amp; LEDs &amp; Infrared"/>
<attribute name="DATASHEET" value="https://www.lcsc.com/datasheet/lcsc_datasheet_2305091500_Hubei-KENTO-Elec-KT-0805W_C34499.pdf"/>
<attribute name="DESC" value="LED"/>
<attribute name="FULL_DESC" value="LED Indication - Discrete"/>
<attribute name="JLC_ROT" value="0"/>
<attribute name="LCSC" value="C34499"/>
<attribute name="MANUFACTURER" value="Hubei KENTO Elec"/>
<attribute name="MPN" value="KT-0805W"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="0805"/>
<attribute name="SOLDER_JOINTS" value="2"/>
<attribute name="SUBCATEGORY" value="Light Emitting Diodes (LED)"/>
<attribute name="VALUE"/>
</element>
<element name="SW601" library="Adom_Library_Master Library" package="3X1_JUMP" value="">
<attribute name="NAME"/>
<attribute name="P1" value="NC"/>
<attribute name="P2" value="nRST"/>
<attribute name="P3" value="GND"/>
</element>
<element name="R2" library="Adom_Library_Master Library" package="3X1_COMPONENT" value="COMPONENT_3X1">
<attribute name="NAME"/>
<attribute name="P1" value="CH4"/>
<attribute name="P1" value="CH4"/>
<attribute name="P2" value="LED4"/>
<attribute name="P2" value="LED4"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="Adom_Library_Master Library" package="3X1_COMPONENT" value="COMPONENT_3X1">
<attribute name="NAME"/>
<attribute name="P1" value="TIS"/>
<attribute name="P1" value="TIS"/>
<attribute name="P2" value="LED4"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="Adom_Library_Master Library" package="3X1_COMPONENT" value="COMPONENT_3X1">
<attribute name="NAME"/>
<attribute name="P1" value="CH3"/>
<attribute name="P1" value="CH3"/>
<attribute name="P2" value="LED3"/>
<attribute name="P2" value="LED3"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="Adom_Library_Master Library" package="3X1_COMPONENT" value="COMPONENT_3X1">
<attribute name="NAME"/>
<attribute name="P1" value="TIS"/>
<attribute name="P2" value="LED3"/>
<attribute name="P2" value="LED3"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="Adom_Library_Master Library" package="3X1_COMPONENT" value="COMPONENT_3X1">
<attribute name="NAME"/>
<attribute name="P1" value="CH2"/>
<attribute name="P1" value="CH2"/>
<attribute name="P2" value="LED2"/>
<attribute name="P2" value="LED2"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="Adom_Library_Master Library" package="3X1_COMPONENT" value="COMPONENT_3X1">
<attribute name="NAME"/>
<attribute name="P1" value="TIS"/>
<attribute name="P1" value="TIS"/>
<attribute name="P2" value="LED2"/>
<attribute name="VALUE"/>
</element>
<element name="R9" library="Adom_Library_Master Library" package="3X1_COMPONENT" value="COMPONENT_3X1">
<attribute name="NAME"/>
<attribute name="P1" value="TIS"/>
<attribute name="P2" value="LED1"/>
<attribute name="P2" value="LED1"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="Adom_Library_Master Library" package="3X1_COMPONENT" value="COMPONENT_3X1">
<attribute name="NAME"/>
<attribute name="P1" value="CH1"/>
<attribute name="P1" value="CH1"/>
<attribute name="P2" value="LED1"/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="Adom JLCPCB Basic Parts Generated - Mar22_2025" package="SODFL3718X115" value="1A INDEP TYP 1k SOD-123FL C64898">
<attribute name="CATEGORY" value="Diodes"/>
<attribute name="DATASHEET" value="https://www.lcsc.com/datasheet/lcsc_datasheet_2407101127_MDD-Microdiode-Semiconductor-SM4007PL_C64898.pdf"/>
<attribute name="DESC" value="1A INDEP TYP 1kV 1.1"/>
<attribute name="FULL_DESC" value="1A Independent Type 1kV 1.1V@1A"/>
<attribute name="JLC_ROT" value="0"/>
<attribute name="LCSC" value="C81598"/>
<attribute name="MANUFACTURER" value="MDD（Microdiode Electronics）"/>
<attribute name="MPN" value="SM4007PL"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="SOD-123FL"/>
<attribute name="SOLDER_JOINTS" value="2"/>
<attribute name="SUBCATEGORY" value="Diodes - General Purpose"/>
<attribute name="VALUE"/>
</element>
<element name="D2" library="Adom JLCPCB Basic Parts Generated - Mar22_2025" package="SODFL3718X115" value="1A INDEP TYP 1k SOD-123FL C64898">
<attribute name="CATEGORY" value="Diodes"/>
<attribute name="DATASHEET" value="https://www.lcsc.com/datasheet/lcsc_datasheet_2407101127_MDD-Microdiode-Semiconductor-SM4007PL_C64898.pdf"/>
<attribute name="DESC" value="1A INDEP TYP 1kV 1.1"/>
<attribute name="FULL_DESC" value="1A Independent Type 1kV 1.1V@1A"/>
<attribute name="JLC_ROT" value="0"/>
<attribute name="LCSC" value="C81598"/>
<attribute name="MANUFACTURER" value="MDD（Microdiode Electronics）"/>
<attribute name="MPN" value="SM4007PL"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="SOD-123FL"/>
<attribute name="SOLDER_JOINTS" value="2"/>
<attribute name="SUBCATEGORY" value="Diodes - General Purpose"/>
<attribute name="VALUE"/>
</element>
<element name="D4" library="Adom JLCPCB Basic Parts Generated - Mar22_2025" package="SODFL3718X115" value="1A INDEP TYP 1k SOD-123FL C64898">
<attribute name="CATEGORY" value="Diodes"/>
<attribute name="DATASHEET" value="https://www.lcsc.com/datasheet/lcsc_datasheet_2407101127_MDD-Microdiode-Semiconductor-SM4007PL_C64898.pdf"/>
<attribute name="DESC" value="1A INDEP TYP 1kV 1.1"/>
<attribute name="FULL_DESC" value="1A Independent Type 1kV 1.1V@1A"/>
<attribute name="JLC_ROT" value="0"/>
<attribute name="LCSC" value="C81598"/>
<attribute name="MANUFACTURER" value="MDD（Microdiode Electronics）"/>
<attribute name="MPN" value="SM4007PL"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="SOD-123FL"/>
<attribute name="SOLDER_JOINTS" value="2"/>
<attribute name="SUBCATEGORY" value="Diodes - General Purpose"/>
<attribute name="VALUE"/>
</element>
<element name="D7" library="Adom JLCPCB Basic Parts Generated - Mar22_2025" package="SODFL3718X115" value="1A INDEP TYP 1k SOD-123FL C64898">
<attribute name="CATEGORY" value="Diodes"/>
<attribute name="DATASHEET" value="https://www.lcsc.com/datasheet/lcsc_datasheet_2407101127_MDD-Microdiode-Semiconductor-SM4007PL_C64898.pdf"/>
<attribute name="DESC" value="1A INDEP TYP 1kV 1.1"/>
<attribute name="FULL_DESC" value="1A Independent Type 1kV 1.1V@1A"/>
<attribute name="JLC_ROT" value="0"/>
<attribute name="LCSC" value="C81598"/>
<attribute name="MANUFACTURER" value="MDD（Microdiode Electronics）"/>
<attribute name="MPN" value="SM4007PL"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="SOD-123FL"/>
<attribute name="SOLDER_JOINTS" value="2"/>
<attribute name="SUBCATEGORY" value="Diodes - General Purpose"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="COSMIIC Library" package="COSMIIC+ADOM_BIG" value="">
</element>
</elements>
<signals>
<signal name="BUSB">
<contactref element="J1" pad="01"/>
<contactref element="MP6" pad="P$1"/>
<contactref element="MP8" pad="P$1"/>
<contactref element="MP50" pad="P$1"/>
</signal>
<signal name="BUSA">
<contactref element="J1" pad="02"/>
<contactref element="MP5" pad="P$1"/>
<contactref element="MP7" pad="P$1"/>
<contactref element="MP51" pad="P$1"/>
</signal>
<signal name="CH2">
<contactref element="J1" pad="03"/>
<contactref element="MP47" pad="P$1"/>
<contactref element="R6" pad="P1"/>
<contactref element="D6" pad="C"/>
<contactref element="D4" pad="1"/>
</signal>
<signal name="CH1">
<contactref element="J1" pad="04"/>
<contactref element="MP48" pad="P$1"/>
<contactref element="R8" pad="P1"/>
<contactref element="D8" pad="C"/>
<contactref element="D7" pad="1"/>
</signal>
<signal name="3V3">
<contactref element="J1" pad="05"/>
<contactref element="MP3" pad="P$1"/>
<contactref element="MP2" pad="P$1"/>
<contactref element="MP43" pad="P$1"/>
</signal>
<signal name="GND">
<contactref element="J1" pad="06"/>
<contactref element="J1" pad="09"/>
<contactref element="J1" pad="26"/>
<contactref element="MP53" pad="P$1"/>
<contactref element="MP55" pad="P$1"/>
<contactref element="MP1" pad="P$1"/>
<contactref element="MP4" pad="P$1"/>
<contactref element="MP60" pad="P$1"/>
<contactref element="MP61" pad="P$1"/>
<contactref element="MP64" pad="P$1"/>
<contactref element="MP65" pad="P$1"/>
<contactref element="MP66" pad="P$1"/>
<contactref element="MP67" pad="P$1"/>
<contactref element="MP68" pad="P$1"/>
<contactref element="MP69" pad="P$1"/>
<contactref element="MP49" pad="P$1"/>
<contactref element="MP44" pad="P$1"/>
<contactref element="MP41" pad="P$1"/>
<contactref element="MP38" pad="P$1"/>
<contactref element="MP35" pad="P$1"/>
<contactref element="MP32" pad="P$1"/>
<contactref element="MP28" pad="P$1"/>
<contactref element="MP25" pad="P$1"/>
<contactref element="MP20" pad="P$1"/>
<contactref element="SW601" pad="P3"/>
</signal>
<signal name="RXCAN">
<contactref element="J1" pad="07"/>
<contactref element="MP39" pad="P$1"/>
</signal>
<signal name="TXCAN">
<contactref element="J1" pad="08"/>
<contactref element="MP40" pad="P$1"/>
</signal>
<signal name="NRESET">
<contactref element="J1" pad="10"/>
<contactref element="MP37" pad="P$1"/>
<contactref element="SW601" pad="P2"/>
</signal>
<signal name="SDATA">
<contactref element="J1" pad="11"/>
<contactref element="MP34" pad="P$1"/>
</signal>
<signal name="SCLOCK">
<contactref element="J1" pad="12"/>
<contactref element="MP33" pad="P$1"/>
</signal>
<signal name="MOSI">
<contactref element="J1" pad="13"/>
<contactref element="MP30" pad="P$1"/>
</signal>
<signal name="SCK">
<contactref element="J1" pad="14"/>
<contactref element="MP31" pad="P$1"/>
</signal>
<signal name="MISO">
<contactref element="J1" pad="15"/>
<contactref element="MP29" pad="P$1"/>
</signal>
<signal name="VIN">
<contactref element="J1" pad="16"/>
<contactref element="MP42" pad="P$1"/>
</signal>
<signal name="TXD0">
<contactref element="J1" pad="17"/>
<contactref element="MP27" pad="P$1"/>
</signal>
<signal name="TDI">
<contactref element="J1" pad="18"/>
<contactref element="MP24" pad="P$1"/>
</signal>
<signal name="TDO">
<contactref element="J1" pad="19"/>
<contactref element="MP23" pad="P$1"/>
</signal>
<signal name="TCK">
<contactref element="J1" pad="20"/>
<contactref element="MP22" pad="P$1"/>
</signal>
<signal name="RXD0">
<contactref element="J1" pad="21"/>
<contactref element="MP26" pad="P$1"/>
</signal>
<signal name="ANODE">
<contactref element="J1" pad="22"/>
<contactref element="MP36" pad="P$1"/>
<contactref element="R1" pad="P2"/>
</signal>
<signal name="TMS">
<contactref element="J1" pad="23"/>
<contactref element="MP21" pad="P$1"/>
</signal>
<signal name="CH3">
<contactref element="J1" pad="24"/>
<contactref element="MP46" pad="P$1"/>
<contactref element="R4" pad="P1"/>
<contactref element="D3" pad="C"/>
<contactref element="D2" pad="1"/>
</signal>
<signal name="CH4">
<contactref element="J1" pad="25"/>
<contactref element="MP45" pad="P$1"/>
<contactref element="R2" pad="P1"/>
<contactref element="D5" pad="C"/>
<contactref element="D1" pad="1"/>
</signal>
<signal name="TISSUE">
<contactref element="MP52" pad="P$1"/>
<contactref element="MP54" pad="P$1"/>
<contactref element="R1" pad="P1"/>
<contactref element="R3" pad="P1"/>
<contactref element="R5" pad="P1"/>
<contactref element="R7" pad="P1"/>
<contactref element="R9" pad="P1"/>
</signal>
<signal name="LED2">
<contactref element="D6" pad="A"/>
<contactref element="D4" pad="2"/>
<contactref element="R6" pad="P2"/>
<contactref element="R7" pad="P2"/>
</signal>
<signal name="LED4">
<contactref element="D5" pad="A"/>
<contactref element="D1" pad="2"/>
<contactref element="R2" pad="P2"/>
<contactref element="R3" pad="P2"/>
</signal>
<signal name="LED3">
<contactref element="D3" pad="A"/>
<contactref element="D2" pad="2"/>
<contactref element="R4" pad="P2"/>
<contactref element="R5" pad="P2"/>
</signal>
<signal name="LED1">
<contactref element="D8" pad="A"/>
<contactref element="D7" pad="2"/>
<contactref element="R8" pad="P2"/>
<contactref element="R9" pad="P2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
